; /****************************************************************************
; * Copyright 2009 Atheros Communications Inc., all rights reserved.          *
; * INF file for Atheros reference designs                                    *
; ****************************************************************************/

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %ATHEROS%
LoutFiles   = layout.inf
CatalogFile = athrext.cat
DriverVer   = 10/05/2009,8.0.0.238

[Manufacturer]
%ATHEROS%     = Atheros, NTX86.6.1, NTX86.6.0
%GIGABYTE%    = Gigabyte, NTX86.6.1, NTX86.6.0

[ControlFlags]
ExcludeFromSelect = *
;
; OS 6.1 Manufacturer section
;
[Atheros.NTX86.6.1]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
;legacy HW Entries
%ATHR.DeviceDesc.1030%     = ATHR_DEV_OS61_1030.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1030168C
%ATHR.DeviceDesc.2030%     = ATHR_DEV_OS61_2030.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2030168C
%ATHR.DeviceDesc.1031%     = ATHR_DEV_OS61_1031.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1031168C
%ATHR.DeviceDesc.2031%     = ATHR_DEV_OS61_2031.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2031168C
%ATHR.DeviceDesc.1041%     = ATHR_DEV_OS61_1041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1041168C
%ATHR.DeviceDesc.2041%     = ATHR_DEV_OS61_2041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2041168C
%ATHR.DeviceDesc.1042%     = ATHR_DEV_OS61_1042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1042168C
%ATHR.DeviceDesc.2042%     = ATHR_DEV_OS61_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2042168C
%ATHR.DeviceDesc.1051%     = ATHR_DEV_OS61_1051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1051168C
%ATHR.DeviceDesc.2051%     = ATHR_DEV_OS61_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2051168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_1052.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_1052168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_2052.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_2052168C
%ATHR.DeviceDesc.1053%     = ATHR_DEV_OS61_1053.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1053168C
%ATHR.DeviceDesc.2053%     = ATHR_DEV_OS61_2053.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2053168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_1054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_1054168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_2054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_2054168C
%ATHR.DeviceDesc.1062%     = ATHR_DEV_OS61_1062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1062168C
%ATHR.DeviceDesc.2062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2062168C
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_1063.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1063168C
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_2063.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2063168C
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3062168C
%ATHR.DeviceDesc.3063%     = ATHR_DEV_OS61_2063.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3063168C
%ATHR.DeviceDesc.3061%     = ATHR_DEV_OS61_2051.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3061168C
%ATHR.DeviceDesc.3065%     = ATHR_DEV_OS61_2052.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3065168C
%ATHR.DeviceDesc.2061%     = ATHR_DEV_OS61_2051.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2061168C
%ATHR.DeviceDesc.1061%     = ATHR_DEV_OS61_1051.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1061168C
%ATHR.DeviceDesc.2065%     = ATHR_DEV_OS61_2052.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2065168C
%ATHR.DeviceDesc.1065%     = ATHR_DEV_OS61_1052.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1065168C
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3067168C
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_3064.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3064168C
%ATHR.DeviceDesc.2055%     = ATHR_DEV_OS61_2055.ndi,     PCI\VEN_168C&DEV_001D&SUBSYS_2055168C
%ATHR.DeviceDesc.2055%     = ATHR_DEV_OS61_1055.ndi,     PCI\VEN_168C&DEV_001D&SUBSYS_1055168C
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1025168C
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1026168C
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2026168C
%ATHR.DeviceDesc.1071%     = ATHR_DEV_OS61_1071.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_1071168C
%ATHR.DeviceDesc.1071%     = ATHR_DEV_OS61_1071.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_2071168C
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_1072168C
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_2072168C
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_3072168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3091168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3092168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3093168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3094168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3095168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3096168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3097168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3098168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3099168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309A168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309B168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309C168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309D168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309F168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2091168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2092168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091PB.ndi,   PCI\VEN_168C&DEV_0029&SUBSYS_2093168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2094168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2096168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2098168C
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30A1168C
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30A2168C
%ATHR.DeviceDesc.30AA%     = ATHR_DEV_OS61_30AA.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AA168C
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AB168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_30A3168C
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_002C&SUBSYS_30A7168C
%ATHR.DeviceDesc.2099%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002D&SUBSYS_2099168C
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002E&SUBSYS_30A4168C
; Customer X
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_A527167D
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_7125144F.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_04291468
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_04301468
; Foxconn
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_04221468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04221468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_04221468.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_04171468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_04221468.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_04181468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_04221468.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_04201468
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_E023105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E023105B
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_OS61_E029105B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_E029105B
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_OS61_E029105B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_1029105B
; Apple
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_0087106B
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_0086106B
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_00000000
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_008F106B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_008F106B
; Linksys
%ATHR.DeviceDesc.1737_g%   = ATHR_DEV_OS61_001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_00531737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_001B.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_00431737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00351731
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00351737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00171737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00251737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1026168C
%ATHR.DeviceDesc.1737_abg% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00361737
; Siemens
%ATHR.DeviceDesc.800118CB% = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_800118CB
%ATHR.DeviceDesc.3070%     = ATHR_DEV_OS61_1042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_307002FA
%ATHR.DeviceDesc.3071%     = ATHR_DEV_OS61_1042.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_307102FA
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_662111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_662111AD
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_662111AD.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_662211AD
;Accton
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_75191113
; AMD
%ATHR.DeviceDesc.90001385% = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_1130168C
; Netgear
%ATHR.DeviceDesc.90001385% = ATHR_DEV_OS61_90001385.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_90001385
%ATHR.DeviceDesc.4B001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4B001385
%ATHR.DeviceDesc.4B001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5B001385
%ATHR.DeviceDesc.5D001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5D001385
%ATHR.DeviceDesc.4D001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4D001385
%ATHR.DeviceDesc.4F001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4F001385
%ATHR.DeviceDesc.5E001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5E001385
%ATHR.DeviceDesc.4D001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5A001385
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_46101385
; OQO
%ATHR.DeviceDesc.2062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1602196f
%ATHR.DeviceDesc.2062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1603196f
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_1604196f
;Lenovo Japan
%ATHR.DeviceDesc.5013%     = ATHR_DEV_OS61_5013.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_0034168c
%ATHR.DeviceDesc.6013%     = ATHR_DEV_OS61_6013.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_0035168c
%ATHR.DeviceDesc.3013%     = ATHR_DEV_OS61_3013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_05891014
%ATHR.DeviceDesc.4013%     = ATHR_DEV_OS61_4013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_058A1014
%ATHR.DeviceDesc.2013%     = ATHR_DEV_OS61_2013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_057E1014
%ATHR.DeviceDesc.1013%     = ATHR_DEV_OS61_1013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_04081468
%ATHR.DeviceDesc.0032168c% = ATHR_DEV_OS61_0032168c.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_0032168c
%ATHR.DeviceDesc.0033168c% = ATHR_DEV_OS61_0033168c.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_0033168c
%ATHR.DeviceDesc.0036%     = ATHR_DEV_OS61_0036.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_0036168c
%ATHR.DeviceDesc.0037%     = ATHR_DEV_OS61_0037.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0037168c
; Lenovo China
%ATHR.DeviceDesc.309917AA% = ATHR_DEV_OS61_309917AA.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309917AA
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_316417AA.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_316417AA
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_309D17AA.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309D17AA
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_309D17AA.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_30A117AA
; IBM
%ATHR.DeviceDesc.0033168c% = ATHR_DEV_OS61_03841014.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_03841014
; Samsung
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7101144F
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7114144F
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7115144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_7131144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_7130144F
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_S001B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7108144F
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_S001B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7116144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_E00B105B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_E00C105B
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_S3067.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_E00E105B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_E00F105B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_E010105B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_7161144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7167144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E025105B
; D-Link
%ATHR.DeviceDesc.DWA642%   = ATHR_DEV_OS61_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A6A1186
%ATHR.DeviceDesc.DWA645%   = ATHR_DEV_OS61_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A0907D1
%ATHR.DeviceDesc.DWA645%   = ATHR_DEV_OS61_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A761186
%ATHR.DeviceDesc.DWA645%   = ATHR_DEV_OS61_3A7B1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A791186
%ATHR.DeviceDesc.DWA542%   = ATHR_DEV_OS61_3A691186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A691186
%ATHR.DeviceDesc.DWA547%   = ATHR_DEV_OS61_3A6D1186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A6B1186
%ATHR.DeviceDesc.DWA547%   = ATHR_DEV_OS61_3A7A1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A781186
%ATHR.DeviceDesc.DWA652%   = ATHR_DEV_OS61_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A6E1186
%ATHR.DeviceDesc.DWA652%   = ATHR_DEV_OS61_3A7B1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A7B1186
%ATHR.DeviceDesc.DWA552%   = ATHR_DEV_OS61_3A6D1186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A6D1186
%ATHR.DeviceDesc.DWA552%   = ATHR_DEV_OS61_3A7A1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A7A1186
%ATHR.DeviceDesc.DWA643%   = ATHR_DEV_OS61_3A6F1186.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_3A6F1186
%ATHR.DeviceDesc.DWA556%   = ATHR_DEV_OS61_3A701186.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_3A701186
%ATHR.DeviceDesc.G650%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A121186
%ATHR.DeviceDesc.G520X%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_32031186
%ATHR.DeviceDesc.G520%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A131186
%ATHR.DeviceDesc.AG520%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A081186
%ATHR.DeviceDesc.AG530%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A141186
%ATHR.DeviceDesc.G630%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A151186
%ATHR.DeviceDesc.G510%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A161186
%ATHR.DeviceDesc.AG650%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A071186
%ATHR.DeviceDesc.AG660%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A631186
%ATHR.DeviceDesc.G680%     = ATHR_DEV_OS61_3A171186.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_3A171186
%ATHR.DeviceDesc.G550%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A181186
%ATHR.DeviceDesc.AG660B%   = ATHR_DEV_OS61_3A171186.ndi, PCI\VEN_168C&DEV_001B&SUBSYS_3A191186
%ATHR.DeviceDesc.AG530B%   = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_3A221186
%ATHR.DeviceDesc.G650P%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A241186
%ATHR.DeviceDesc.G520P%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A231186
%ATHR.DeviceDesc.WDA1320%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A1D1186
%ATHR.DeviceDesc.WDA2320%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A1B1186
%ATHR.DeviceDesc.DWA520%   = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A731186
%ATHR.DeviceDesc.DWA620%   = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A741186
%ATHR.DeviceDesc.CWNA2330% = ATHR_DEV_OS61_3A171186.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_3A1A1186
%ATHR.DeviceDesc.CWNA1330% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A1C1186
%ATHR.DeviceDesc.CWNA1330% = ATHR_DEV_OS61_3A171186.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_3A1C1186
%ATHR.DeviceDesc.CG650%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_32021186
%ATHR.DeviceDesc.CG630%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3B081186
%ATHR.DeviceDesc.CG630%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3B081186
; Alpha/ATKK
%ATIWC.DeviceDesc.ATICB%   = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_12041259
%ATIWC.DeviceDesc.ATIPC%   = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_12031259
; Motion Computing
%ATHR.DeviceDesc.3061%     = ATHR_DEV_OS61_7111144F.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_7111144F
; Azurewave
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_10341A3B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10261A3B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10601A3B
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_10241A3B.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_10241A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_10671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10671A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_10711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10711A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_10711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10811A3B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_10891A3B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_20371A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_20371A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_10671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10901A3B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_20371A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_11061A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_1A671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1A671A3B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_1A891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_1A891A3B
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_OS61_11121A3B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_11121A3B
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_OS61_11121A3B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_1A121A3B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10331A3B
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_20361A3B
%ATHR.DeviceDesc.30AA%     = ATHR_DEV_OS61_30AA.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_20371A3B
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_2C371A3B
; Huawei
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5003485
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5013485
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_663111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5023485
; Panasonic
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_1C711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1C711A3B
; QMI    
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_01121A32                        
%ATHR.DeviceDesc.3065%     = ATHR_DEV_OS61_01001A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01001A32
%ATHR.DeviceDesc.3063%     = ATHR_DEV_OS61_01001A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_02001A32
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_05021A32
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03011A32
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_05041A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_21081A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01051A32 
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_03051A32.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_03051A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_2A97103C
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_01121A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01121A32
; Arcadyan
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_C6011113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_D8111113.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_D8111113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_03051A32.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_F6111113
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_C8221113
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_D8221113
; Askey/Compal
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7168144F
; LiteOn
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_630311AD
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_631311AD
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_633311AD
%ATHR.DeviceDesc.2061%     = ATHR_DEV_OS61_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_530111AD
%ATHR.DeviceDesc.2062%     = ATHR_DEV_OS61_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_540111AD
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_660311AD
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_661311AD
; Acer
%ATHR.DeviceDesc.E006105B% = ATHR_DEV_OS61_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_660011AD 
%ATHR.DeviceDesc.E006105B% = ATHR_DEV_OS61_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E006105B
%ATHR.DeviceDesc.E006105B% = ATHR_DEV_OS61_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03031A32
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_OS61_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E01F105B
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_OS61_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_663211AD
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_OS61_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03061A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01081A32   
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04281468
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E008105B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E00D105B
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_663111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_663111AD
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_635311AD
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_660311AD
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_663111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E016105B
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_663111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E022105B
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_OS61_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309D185F
; Toshiba
%ATHR.DeviceDesc.2041%     = ATHR_DEV_OS61_2041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7064144F
%ATHR.DeviceDesc.2042%     = ATHR_DEV_OS61_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7065144F
%ATHR.DeviceDesc.2051%     = ATHR_DEV_OS61_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7084144F
%ATHR.DeviceDesc.2051%     = ATHR_DEV_OS61_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7088144F
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_001B.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_7092144F
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_2054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_7094144F
%ATHR.DeviceDesc.3063%     = ATHR_DEV_OS61_2063.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7096144F
%ATHR.DeviceDesc.3065%     = ATHR_DEV_OS61_2052.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7106144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7128144f
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_001A.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_04271468
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_001B.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_04251468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_04261468
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_7125144F.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_7125144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_042A1468
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E004105B
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E009105B
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7136144F
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7154144F
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7141144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_41051A32
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43011A32  
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43031A32
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E012105B
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E013105B
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E015105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_E014105B
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7158144F
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7156144F
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7157144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_7159144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_632311AD
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_662011AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_650211AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_653211AD
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_661011AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_651211AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_652211AD
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_661111AD
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_661211AD
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_660111AD
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7163144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_7164144F
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E019105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_E01A105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_43051A32
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43061A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_A6011113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_E6111113
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E6221113
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_D6221113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_E8111113
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_F8221113
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_A8221113
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_B8221113
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_45071A32
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_65071A32
; Sony
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_E007105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E007105B
%ATHR.DeviceDesc.04231468% = ATHR_DEV_OS61_E000105B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E000105B
%ATHR.DeviceDesc.04231468% = ATHR_DEV_OS61_E002105B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E002105B
%ATHR.DeviceDesc.04061468% = ATHR_DEV_OS61_04061468.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_04061468
%ATHR.DeviceDesc.04071468% = ATHR_DEV_OS61_04061468.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_04071468 
%ATHR.DeviceDesc.04231468% = ATHR_DEV_OS61_04231468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04231468 
%ATHR.DeviceDesc.04231468% = ATHR_DEV_OS61_04231468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_0423168C
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_S30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E017105B
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_SS30A1.ndi,   PCI\VEN_168C&DEV_002E&SUBSYS_E030105B
; HP Desktop
%ATHR.DeviceDesc.2A5F103C% = ATHR_DEV_OS61_2A5F103C.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_2A5F103C
%ATHR.DeviceDesc.500011AD% = ATHR_DEV_OS61_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_500011AD
%ATHR.DeviceDesc.500111AD% = ATHR_DEV_OS61_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_500111AD
%ATHR.DeviceDesc.1000168c% = ATHR_DEV_OS61_1000168C.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1000168C
%ATHR.DeviceDesc.1000168c% = ATHR_DEV_OS61_1001168C.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1001168C
; Asus
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7112144f
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7137144F
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_7122144F
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_1071.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_7132144F
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_1071.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_2072144F
; Sharp(Mitac)
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7138144F 
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7139144F
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7140144F 
; Fujitsu
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_13C010CF.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_13C010CF
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_147C10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_147C10CF
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_147D10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_147D10CF
%ATHR.DeviceDesc.1071%     = ATHR_DEV_OS61_13C010CF.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_147E10CF
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123410CF
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123510CF
%ATHR.DeviceDesc.10CF%     = ATHR_DEV_OS61_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123610CF
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_F013.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_132910CF
%ATHR.DeviceDesc.10CF%     = ATHR_DEV_OS61_F013.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_134F10CF
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_F013C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_139C10CF
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_F01C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_142E10CF
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_153710CF.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_153710CF
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_147D10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_153610CF
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_153710CF.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_158F10CF
; WNC
%ATHR.DeviceDesc.CM9%	   = ATHR_DEV_OS61_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1012185F
; TPLINK
%ATHR.DeviceDesc.1ACE%     = ATHR_DEV_OS61_T3091.ndi,    PCI\VEN_168C&DEV_0029&SUBSYS_92231ACE
; Pegatron
%ATHR.DeviceDesc.00341B0A% = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_00341B0A
; Belkin
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_701D1799
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_700D1799
%ATHR.DeviceDesc.F6D3000%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_30001799
%ATHR.DeviceDesc.F6D3000%  = ATHR_DEV_OS61_001B.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_30001799
%ATHR.DeviceDesc.80111799% = ATHR_DEV_OS61_80111799.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_80111799
; NEC 
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_N2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_102010E9
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_N2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_102510E9
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_N3072.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_102210E9
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_N3073.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_102610E9
; IO Data
%ATHR.DeviceDesc.D05B10FC% = ATHR_DEV_OS61_D05B10FC.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_D05B10FC
[Gigabyte.NTX86.6.1]
%GIGA.DeviceDesc.E801%     = GIGA_DEV_OS61_E801.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E8011458
%GIGA.DeviceDesc.E811%     = GIGA_DEV_OS61_E811.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E8111458
%GIGA.DeviceDesc.E814%     = GIGA_DEV_OS61_E814.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E8141458
%GIGA.DeviceDesc.0013%     = GIGA_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E9011458
%GIGA.DeviceDesc.E901%     = GIGA_DEV_OS61_E901.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_E9011458
%GIGA.DeviceDesc.E911%     = GIGA_DEV_OS61_E911.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E9111458
%GIGA.DeviceDesc.E912%     = GIGA_DEV_OS61_E912.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E9121458
%GIGA.DeviceDesc.E913%     = GIGA_DEV_OS61_E913.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_E9131458
%GIGA.DeviceDesc.E917%     = GIGA_DEV_OS61_E917.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_E9171458
%GIGA.DeviceDesc.E815%     = GIGA_DEV_OS61_E914.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_E8151458
%GIGA.DeviceDesc.E914%     = GIGA_DEV_OS61_E914.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_E9141458
%GIGA.DeviceDesc.E915%     = GIGA_DEV_OS61_E914.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_E9151458
%GIGA.DeviceDesc.E916%     = GIGA_DEV_OS61_E916.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_E9161458
%GIGA.DeviceDesc.E918%     = GIGA_DEV_OS61_E918.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_E9181458
%GIGA.DeviceDesc.E9191458% = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E9191458 
;
; Vista Manufacturer section
;
[Atheros.NTX86.6.0]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
;legacy HW Entries
%ATHR.DeviceDesc.1030%     = ATHR_DEV_1030.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1030168C
%ATHR.DeviceDesc.2030%     = ATHR_DEV_2030.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2030168C
%ATHR.DeviceDesc.1031%     = ATHR_DEV_1031.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1031168C
%ATHR.DeviceDesc.2031%     = ATHR_DEV_2031.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2031168C
%ATHR.DeviceDesc.1041%     = ATHR_DEV_1041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1041168C
%ATHR.DeviceDesc.2041%     = ATHR_DEV_2041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2041168C
%ATHR.DeviceDesc.1042%     = ATHR_DEV_1042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1042168C
%ATHR.DeviceDesc.2042%     = ATHR_DEV_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2042168C
%ATHR.DeviceDesc.1051%     = ATHR_DEV_1051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1051168C
%ATHR.DeviceDesc.2051%     = ATHR_DEV_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2051168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_1052.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_1052168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_2052.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_2052168C
%ATHR.DeviceDesc.1053%     = ATHR_DEV_1053.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1053168C
%ATHR.DeviceDesc.2053%     = ATHR_DEV_2053.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2053168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_1054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_1054168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_2054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_2054168C
%ATHR.DeviceDesc.1062%     = ATHR_DEV_1062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1062168C
%ATHR.DeviceDesc.2062%     = ATHR_DEV_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2062168C
%ATHR.DeviceDesc.001B%     = ATHR_DEV_1063.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1063168C
%ATHR.DeviceDesc.001B%     = ATHR_DEV_2063.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2063168C
%ATHR.DeviceDesc.3062%     = ATHR_DEV_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3062168C
%ATHR.DeviceDesc.3063%     = ATHR_DEV_2063.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3063168C
%ATHR.DeviceDesc.3061%     = ATHR_DEV_2051.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3061168C
%ATHR.DeviceDesc.3065%     = ATHR_DEV_2052.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3065168C
%ATHR.DeviceDesc.2061%     = ATHR_DEV_2051.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2061168C
%ATHR.DeviceDesc.1061%     = ATHR_DEV_1051.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1061168C
%ATHR.DeviceDesc.2065%     = ATHR_DEV_2052.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2065168C
%ATHR.DeviceDesc.1065%     = ATHR_DEV_1052.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1065168C
%ATHR.DeviceDesc.3067%     = ATHR_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3067168C
%ATHR.DeviceDesc.3067%     = ATHR_DEV_3064.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3064168C
%ATHR.DeviceDesc.2055%     = ATHR_DEV_2055.ndi,     PCI\VEN_168C&DEV_001D&SUBSYS_2055168C
%ATHR.DeviceDesc.2055%     = ATHR_DEV_1055.ndi,     PCI\VEN_168C&DEV_001D&SUBSYS_1055168C
%ATHR.DeviceDesc.0013%     = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1025168C
%ATHR.DeviceDesc.0013%     = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1026168C
%ATHR.DeviceDesc.0013%     = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2026168C
%ATHR.DeviceDesc.1071%     = ATHR_DEV_1071.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_1071168C
%ATHR.DeviceDesc.1071%     = ATHR_DEV_1071.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_2071168C
%ATHR.DeviceDesc.3072%     = ATHR_DEV_3072.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_1072168C
%ATHR.DeviceDesc.3072%     = ATHR_DEV_3072.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_2072168C
%ATHR.DeviceDesc.3072%     = ATHR_DEV_3072.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_3072168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3091168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3092168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3093168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3094168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3095168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3096168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3097168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3098168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3099168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309A168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309B168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309C168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309D168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309F168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2091168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2092168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_3091PB.ndi,   PCI\VEN_168C&DEV_0029&SUBSYS_2093168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2094168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2096168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2098168C
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30A1168C
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30A2168C
%ATHR.DeviceDesc.30AA%     = ATHR_DEV_30AA.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AA168C
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AB168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_30A3168C
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_001C.ndi,     PCI\VEN_168C&DEV_002C&SUBSYS_30A7168C
%ATHR.DeviceDesc.2099%     = ATHR_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002D&SUBSYS_2099168C
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002E&SUBSYS_30A4168C
; Customer X
%ATHR.DeviceDesc.0013%     = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_A527167D
%ATHR.DeviceDesc.3072%     = ATHR_DEV_7125144F.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_04291468
%ATHR.DeviceDesc.3072%     = ATHR_DEV_3072.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_04301468
; Foxconn
%ATHR.DeviceDesc.3062%     = ATHR_DEV_04221468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04221468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_04221468.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_04171468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_04221468.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_04181468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_04221468.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_04201468
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_E023105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E023105B
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_E029105B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_E029105B
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_E029105B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_1029105B
; Apple
%ATHR.DeviceDesc.3072%     = ATHR_DEV_3072.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_0087106B
%ATHR.DeviceDesc.3062%     = ATHR_DEV_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_0086106B
%ATHR.DeviceDesc.3072%     = ATHR_DEV_3072.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_00000000
%ATHR.DeviceDesc.3091%     = ATHR_DEV_008F106B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_008F106B
; Linksys
%ATHR.DeviceDesc.1737_g%   = ATHR_DEV_001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_00531737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_001B.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_00431737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00351731
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00351737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00171737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00251737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1026168C
%ATHR.DeviceDesc.1737_abg% = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00361737
; Siemens
%ATHR.DeviceDesc.800118CB% = ATHR_DEV_3072.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_800118CB
%ATHR.DeviceDesc.3070%     = ATHR_DEV_1042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_307002FA
%ATHR.DeviceDesc.3071%     = ATHR_DEV_1042.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_307102FA
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_662111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_662111AD
%ATHR.DeviceDesc.3091%     = ATHR_DEV_662111AD.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_662211AD
; Accton
%ATHR.DeviceDesc.3062%     = ATHR_DEV_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_75191113
; AMD
%ATHR.DeviceDesc.90001385% = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_1130168C
; Netgear
%ATHR.DeviceDesc.90001385% = ATHR_DEV_90001385.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_90001385
%ATHR.DeviceDesc.4B001385% = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4B001385
%ATHR.DeviceDesc.4B001385% = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5B001385
%ATHR.DeviceDesc.5D001385% = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5D001385
%ATHR.DeviceDesc.4D001385% = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4D001385
%ATHR.DeviceDesc.4F001385% = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4F001385
%ATHR.DeviceDesc.5E001385% = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5E001385
%ATHR.DeviceDesc.4D001385% = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5A001385
%ATHR.DeviceDesc.0013%     = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_46101385
; OQO
%ATHR.DeviceDesc.2062%     = ATHR_DEV_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1602196f
%ATHR.DeviceDesc.2062%     = ATHR_DEV_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1603196f
%ATHR.DeviceDesc.3062%     = ATHR_DEV_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_1604196f
; Lenovo Japan
%ATHR.DeviceDesc.5013%     = ATHR_DEV_5013.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_0034168c
%ATHR.DeviceDesc.6013%     = ATHR_DEV_6013.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_0035168c
%ATHR.DeviceDesc.3013%     = ATHR_DEV_3013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_05891014
%ATHR.DeviceDesc.4013%     = ATHR_DEV_4013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_058A1014
%ATHR.DeviceDesc.2013%     = ATHR_DEV_2013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_057E1014
%ATHR.DeviceDesc.1013%     = ATHR_DEV_1013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_04081468
%ATHR.DeviceDesc.0032168c% = ATHR_DEV_0032168c.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_0032168c
%ATHR.DeviceDesc.0033168c% = ATHR_DEV_0033168c.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_0033168c
%ATHR.DeviceDesc.0036%     = ATHR_DEV_0036.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_0036168c
%ATHR.DeviceDesc.0037%     = ATHR_DEV_0037.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0037168c
;Lenovo China
%ATHR.DeviceDesc.309917AA% = ATHR_DEV_309917AA.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309917AA
%ATHR.DeviceDesc.3067%     = ATHR_DEV_316417AA.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_316417AA
%ATHR.DeviceDesc.3091%     = ATHR_DEV_309D17AA.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309D17AA
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_309D17AA.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_30A117AA
; IBM
%ATHR.DeviceDesc.0033168c% = ATHR_DEV_03841014.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_03841014
; Samsung
%ATHR.DeviceDesc.001A%     = ATHR_DEV_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7101144F
%ATHR.DeviceDesc.001A%     = ATHR_DEV_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7114144F
%ATHR.DeviceDesc.001A%     = ATHR_DEV_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7115144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_7131144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_7130144F
%ATHR.DeviceDesc.001B%     = ATHR_DEV_S001B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7108144F
%ATHR.DeviceDesc.001B%     = ATHR_DEV_S001B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7116144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_E00B105B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_E00C105B
%ATHR.DeviceDesc.001B%     = ATHR_DEV_S3067.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_E00E105B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_E00F105B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_E010105B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_7161144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7167144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E025105B
; D-Link
%ATHR.DeviceDesc.DWA642%   = ATHR_DEV_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A6A1186
%ATHR.DeviceDesc.DWA645%   = ATHR_DEV_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A0907D1
%ATHR.DeviceDesc.DWA645%   = ATHR_DEV_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A761186
%ATHR.DeviceDesc.DWA645%   = ATHR_DEV_3A7B1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A791186
%ATHR.DeviceDesc.DWA542%   = ATHR_DEV_3A691186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A691186
%ATHR.DeviceDesc.DWA547%   = ATHR_DEV_3A6D1186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A6B1186
%ATHR.DeviceDesc.DWA547%   = ATHR_DEV_3A7A1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A781186
%ATHR.DeviceDesc.DWA652%   = ATHR_DEV_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A6E1186
%ATHR.DeviceDesc.DWA652%   = ATHR_DEV_3A7B1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A7B1186
%ATHR.DeviceDesc.DWA552%   = ATHR_DEV_3A6D1186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A6D1186
%ATHR.DeviceDesc.DWA552%   = ATHR_DEV_3A7A1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A7A1186
%ATHR.DeviceDesc.DWA643%   = ATHR_DEV_3A6F1186.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_3A6F1186
%ATHR.DeviceDesc.DWA556%   = ATHR_DEV_3A701186.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_3A701186
%ATHR.DeviceDesc.G650%     = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A121186
%ATHR.DeviceDesc.G520X%    = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_32031186
%ATHR.DeviceDesc.G520%     = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A131186
%ATHR.DeviceDesc.AG520%    = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A081186
%ATHR.DeviceDesc.AG530%    = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A141186
%ATHR.DeviceDesc.G630%     = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A151186
%ATHR.DeviceDesc.G510%     = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A161186
%ATHR.DeviceDesc.AG650%    = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A071186
%ATHR.DeviceDesc.AG660%    = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A631186
%ATHR.DeviceDesc.G680%     = ATHR_DEV_3A171186.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_3A171186
%ATHR.DeviceDesc.G550%     = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A181186
%ATHR.DeviceDesc.AG660B%   = ATHR_DEV_3A171186.ndi, PCI\VEN_168C&DEV_001B&SUBSYS_3A191186
%ATHR.DeviceDesc.AG530B%   = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_3A221186
%ATHR.DeviceDesc.G650P%    = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A241186
%ATHR.DeviceDesc.G520P%    = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A231186
%ATHR.DeviceDesc.WDA1320%  = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A1D1186
%ATHR.DeviceDesc.WDA2320%  = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A1B1186
%ATHR.DeviceDesc.DWA520%   = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A731186
%ATHR.DeviceDesc.DWA620%   = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A741186
%ATHR.DeviceDesc.CWNA2330% = ATHR_DEV_3A171186.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_3A1A1186
%ATHR.DeviceDesc.CWNA1330% = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A1C1186
%ATHR.DeviceDesc.CWNA1330% = ATHR_DEV_3A171186.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_3A1C1186
%ATHR.DeviceDesc.CG650%    = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_32021186
%ATHR.DeviceDesc.CG630%    = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3B081186
%ATHR.DeviceDesc.CG630%    = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3B081186
; Alpha/ATKK
%ATIWC.DeviceDesc.ATICB%   = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_12041259
%ATIWC.DeviceDesc.ATIPC%   = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_12031259
; Motion Computing
%ATHR.DeviceDesc.3061%     = ATHR_DEV_7111144F.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_7111144F
; Azurewave
%ATHR.DeviceDesc.3067%     = ATHR_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_10341A3B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10261A3B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10601A3B
%ATHR.DeviceDesc.3072%     = ATHR_DEV_10241A3B.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_10241A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_10671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10671A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_10711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10711A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_10711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10811A3B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_10891A3B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_20371A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_20371A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_10671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10901A3B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_20371A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_11061A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_1A671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1A671A3B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_1A891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_1A891A3B
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_11121A3B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_11121A3B
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_11121A3B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_1A121A3B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10331A3B
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_20361A3B
%ATHR.DeviceDesc.30AA%     = ATHR_DEV_30AA.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_20371A3B
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_2C371A3B
; Huawei
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5003485
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5013485
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_663111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5023485
; Panasonic
%ATHR.DeviceDesc.3091%     = ATHR_DEV_1C711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1C711A3B
; QMI        
%ATHR.DeviceDesc.0013%     = ATHR_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_01121A32                     
%ATHR.DeviceDesc.3065%     = ATHR_DEV_01001A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01001A32
%ATHR.DeviceDesc.3063%     = ATHR_DEV_01001A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_02001A32
%ATHR.DeviceDesc.3072%     = ATHR_DEV_03011A32.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_05021A32
%ATHR.DeviceDesc.3091%     = ATHR_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03011A32
%ATHR.DeviceDesc.3091%     = ATHR_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_05041A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_21081A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01051A32
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_03051A32.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_03051A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_2A97103C
%ATHR.DeviceDesc.3067%     = ATHR_DEV_01121A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01121A32
; Arcadyan
%ATHR.DeviceDesc.3067%     = ATHR_DEV_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_C6011113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_D8111113.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_D8111113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_03051A32.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_F6111113
%ATHR.DeviceDesc.3091%     = ATHR_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_C8221113 
%ATHR.DeviceDesc.3091%     = ATHR_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_D8221113
; Askey/Compal
%ATHR.DeviceDesc.3091%     = ATHR_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7168144F
; LiteOn
%ATHR.DeviceDesc.3067%     = ATHR_DEV_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_630311AD
%ATHR.DeviceDesc.3067%     = ATHR_DEV_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_631311AD
%ATHR.DeviceDesc.3067%     = ATHR_DEV_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_633311AD
%ATHR.DeviceDesc.2061%     = ATHR_DEV_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_530111AD
%ATHR.DeviceDesc.2062%     = ATHR_DEV_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_540111AD
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_660311AD
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_661311AD
; Acer
%ATHR.DeviceDesc.E006105B% = ATHR_DEV_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_660011AD 
%ATHR.DeviceDesc.E006105B% = ATHR_DEV_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E006105B
%ATHR.DeviceDesc.E006105B% = ATHR_DEV_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03031A32 
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E01F105B
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_663211AD
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03061A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01081A32  
%ATHR.DeviceDesc.3067%     = ATHR_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04281468
%ATHR.DeviceDesc.3067%     = ATHR_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E008105B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E00D105B
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_663111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_663111AD
%ATHR.DeviceDesc.3067%     = ATHR_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_635311AD
%ATHR.DeviceDesc.3067%     = ATHR_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_660311AD
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_663111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E016105B
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_663111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E022105B
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309D185F
; Toshiba
%ATHR.DeviceDesc.2041%     = ATHR_DEV_2041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7064144F
%ATHR.DeviceDesc.2042%     = ATHR_DEV_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7065144F
%ATHR.DeviceDesc.2051%     = ATHR_DEV_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7084144F
%ATHR.DeviceDesc.2051%     = ATHR_DEV_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7088144F
%ATHR.DeviceDesc.001B%     = ATHR_DEV_001B.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_7092144F
%ATHR.DeviceDesc.001A%     = ATHR_DEV_2054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_7094144F
%ATHR.DeviceDesc.3063%     = ATHR_DEV_2063.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7096144F
%ATHR.DeviceDesc.3065%     = ATHR_DEV_2052.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7106144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7128144f
%ATHR.DeviceDesc.001A%     = ATHR_DEV_001A.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_04271468
%ATHR.DeviceDesc.001B%     = ATHR_DEV_001B.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_04251468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_04261468
%ATHR.DeviceDesc.3072%     = ATHR_DEV_7125144F.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_7125144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_042A1468
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E004105B
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E009105B
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7136144F
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7154144F
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7141144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_41051A32
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43011A32  
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43031A32
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E012105B
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E013105B
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E015105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_E014105B
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7158144F
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7156144F
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7157144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_7159144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_632311AD
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_662011AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_650211AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_653211AD
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_661011AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_651211AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_652211AD
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_661111AD
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_661211AD
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_660111AD
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7163144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_7164144F
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E019105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_E01A105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_43051A32
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43061A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_A6011113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_E6111113
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E6221113
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_D6221113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_E8111113
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_F8221113
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_A8221113
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_B8221113
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_45071A32
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_65071A32
; Sony
%ATHR.DeviceDesc.3091%     = ATHR_DEV_E007105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E007105B
%ATHR.DeviceDesc.04231468% = ATHR_DEV_E000105B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E000105B
%ATHR.DeviceDesc.04231468% = ATHR_DEV_E002105B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E002105B
%ATHR.DeviceDesc.04061468% = ATHR_DEV_04061468.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_04061468
%ATHR.DeviceDesc.04071468% = ATHR_DEV_04061468.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_04071468 
%ATHR.DeviceDesc.04231468% = ATHR_DEV_04231468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04231468 
%ATHR.DeviceDesc.04231468% = ATHR_DEV_04231468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_0423168C
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_S30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E017105B
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_SS30A1.ndi,   PCI\VEN_168C&DEV_002E&SUBSYS_E030105B
; HP Desktop
%ATHR.DeviceDesc.2A5F103C% = ATHR_DEV_2A5F103C.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_2A5F103C
%ATHR.DeviceDesc.500011AD% = ATHR_DEV_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_500011AD
%ATHR.DeviceDesc.500111AD% = ATHR_DEV_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_500111AD
%ATHR.DeviceDesc.1000168c% = ATHR_DEV_1000168C.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1000168C
%ATHR.DeviceDesc.1000168c% = ATHR_DEV_1001168C.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1001168C
; Asus
%ATHR.DeviceDesc.3062%     = ATHR_DEV_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7112144f
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7137144F
%ATHR.DeviceDesc.3072%     = ATHR_DEV_3072.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_7122144F
%ATHR.DeviceDesc.3072%     = ATHR_DEV_1071.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_7132144F
%ATHR.DeviceDesc.3072%     = ATHR_DEV_1071.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_2072144F
; Sharp(Mitac)
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7138144F 
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7139144F
%ATHR.DeviceDesc.3091%     = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7140144F 
; Fujitsu
%ATHR.DeviceDesc.3072%     = ATHR_DEV_13C010CF.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_13C010CF
%ATHR.DeviceDesc.3091%     = ATHR_DEV_147C10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_147C10CF
%ATHR.DeviceDesc.3091%     = ATHR_DEV_147D10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_147D10CF
%ATHR.DeviceDesc.1071%     = ATHR_DEV_13C010CF.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_147E10CF
%ATHR.DeviceDesc.0013%     = ATHR_DEV_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123410CF
%ATHR.DeviceDesc.0013%     = ATHR_DEV_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123510CF
%ATHR.DeviceDesc.10CF%     = ATHR_DEV_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123610CF
%ATHR.DeviceDesc.001B%     = ATHR_DEV_F013.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_132910CF
%ATHR.DeviceDesc.10CF%     = ATHR_DEV_F013.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_134F10CF
%ATHR.DeviceDesc.3062%     = ATHR_DEV_F013C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_139C10CF
%ATHR.DeviceDesc.3067%     = ATHR_DEV_F01C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_142E10CF
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_153710CF.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_153710CF
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_147D10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_153610CF
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_153710CF.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_158F10CF
; WNC
%ATHR.DeviceDesc.CM9%	   = ATHR_DEV_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1012185F
; TPLINK
%ATHR.DeviceDesc.1ACE%     = ATHR_DEV_T3091.ndi,    PCI\VEN_168C&DEV_0029&SUBSYS_92231ACE
; Pegatron
%ATHR.DeviceDesc.00341B0A% = ATHR_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_00341B0A
; Belkin
%ATHR.DeviceDesc.001A%     = ATHR_DEV_001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_701D1799
%ATHR.DeviceDesc.001A%     = ATHR_DEV_001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_700D1799
%ATHR.DeviceDesc.F6D3000%  = ATHR_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_30001799
%ATHR.DeviceDesc.F6D3000%  = ATHR_DEV_001B.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_30001799
%ATHR.DeviceDesc.80111799% = ATHR_DEV_80111799.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_80111799
; NEC 
%ATHR.DeviceDesc.3062%     = ATHR_DEV_N2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_102010E9
%ATHR.DeviceDesc.3062%     = ATHR_DEV_N2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_102510E9
%ATHR.DeviceDesc.3072%     = ATHR_DEV_N3072.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_102210E9
%ATHR.DeviceDesc.3072%     = ATHR_DEV_N3073.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_102610E9
; IO Data
%ATHR.DeviceDesc.D05B10FC% = ATHR_DEV_D05B10FC.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_D05B10FC
[Gigabyte.NTX86.6.0]
%GIGA.DeviceDesc.E801%     = GIGA_DEV_E801.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E8011458
%GIGA.DeviceDesc.E811%     = GIGA_DEV_E811.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E8111458
%GIGA.DeviceDesc.E814%     = GIGA_DEV_E814.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E8141458
%GIGA.DeviceDesc.0013%     = GIGA_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E9011458
%GIGA.DeviceDesc.E901%     = GIGA_DEV_E901.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_E9011458
%GIGA.DeviceDesc.E911%     = GIGA_DEV_E911.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E9111458
%GIGA.DeviceDesc.E912%     = GIGA_DEV_E912.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E9121458
%GIGA.DeviceDesc.E913%     = GIGA_DEV_E913.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_E9131458
%GIGA.DeviceDesc.E917%     = GIGA_DEV_E917.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_E9171458
%GIGA.DeviceDesc.E815%     = GIGA_DEV_E914.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_E8151458
%GIGA.DeviceDesc.E914%     = GIGA_DEV_E914.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_E9141458
%GIGA.DeviceDesc.E915%     = GIGA_DEV_E914.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_E9151458
%GIGA.DeviceDesc.E916%     = GIGA_DEV_E916.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_E9161458
%GIGA.DeviceDesc.E918%     = GIGA_DEV_E918.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_E9181458
%GIGA.DeviceDesc.E9191458% = ATHR_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E9191458 
;
; OS 6.1 Manufacturer section
;
[GIGA_DEV_OS61_E801.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E801.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E801.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E811.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E811.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E811.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E814.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E814.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E814.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_0013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_0013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_0013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E901.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E901.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E901.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E911.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E911.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E911.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E912.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E912.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E912.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E913.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E913.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E913.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E917.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E917.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E917.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E918.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E918.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E918.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E914.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer_GigaByte.reg, customer_GigaByteLed0.reg, 5416.antennacontrols.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E914.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E914.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E916.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer_GigaByte.reg, customer_GigaByteLed1.reg, 5416.antennacontrols.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E916.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E916.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_0013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_0013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_0013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_001A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_001A.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_001A.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_001B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_001B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_001B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_001C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_001C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_001C.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_6313.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cemspecled_func1_3.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_6313.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_6313.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3064.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3064.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3064.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1055.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, gpioled.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1055.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1055.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2055.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2055.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2055.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1030.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1030.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1030.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2030.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2030.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2030.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1031.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1031.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1031.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2031.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2031.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2031.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1041.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1041.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1041.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2041.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2041.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2041.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1042.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1042.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1042.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2042.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2042.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2042.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1051.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1051.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1051.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2051.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2051.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2051.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_7111144F.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, expresscardaspmoff.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_7111144F.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_7111144F.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1052.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1052.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1052.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2052.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2052.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2052.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_01001A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer9Led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_01001A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_01001A32.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1053.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1053.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1053.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2053.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2053.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2053.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1054.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1054.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1054.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2054.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2054.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2054.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1062.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1062.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1062.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2062.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2062.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2062.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1063.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1063.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1063.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2063.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2063.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2063.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1071.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1071.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1071.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_90001385.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, expresscardaspmoff.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_90001385.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_90001385.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2A5F103C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer2.11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2A5F103C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2A5F103C.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_11AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_11AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_11AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3072.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3072.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3072.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_10671A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htWepTkipOpt.reg, htAdhoc.reg, indicaterxlinkspeed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_10671A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_10671A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1A671A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1A671A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1A671A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_10711A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htEnableWepTkip.reg, htAdhoc.reg, d3forcel1disable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_10711A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_10711A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1C711A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, 5416.bandselect.reg, htEnableWepTkip.reg, htAdhoc.reg, d3forcel1disable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1C711A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1C711A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_03011A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_03011A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_03011A32.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3091.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3091.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3091.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_008F106B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_008F106B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_008F106B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_309D17AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, Customer15a.led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_309D17AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_309D17AA.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_316417AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, Customer15b.led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_316417AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_316417AA.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_7136144F.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, merlinshiftdelay.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_7136144F.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_7136144F.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_D05B10FC.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, customer_IODATA.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_D05B10FC.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_D05B10FC.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_T3091.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, pcibusconfig.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_T3091.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_T3091.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_309917AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_309917AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_309917AA.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A1.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_660311AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cemspecled_func1_4.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_660311AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_660311AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, triggerlevelkiteonly.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30AA.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30AB.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, janusda.reg, triggerlevelkiteonly.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30AB.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30AB.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A1a.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A1a.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A1a.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E023105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cemspecled_func1_1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E023105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E023105B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E029105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cemspecled_func1_1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E029105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E029105B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_11121A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cemspecled_func1_1.reg, d3forcel1disablekite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_11121A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_11121A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_662111AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_662111AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_662111AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3091PB.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, pushbutton.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3091PB.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3091PB.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1000168C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer2merlin.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1000168C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1000168C.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1001168C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer2.11n.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1001168C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1001168C.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3091SF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer_Samsung.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3091SF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3091SF.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_03051A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_03051A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_03051A32.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_D8111113.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htAdhoc.reg, d3forcel1disablekite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_D8111113.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_D8111113.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_10891A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htWepTkipOpt.reg, htAdhoc.reg, wirelessmodeselectkite.reg, triggerlevelkiteonly.reg, d3forcel1disablekite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_10891A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_10891A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_20371A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htEnableWepTkip.reg, htAdhoc.reg, wirelessmodeselectkite.reg, d3forcel1disablekite.reg, triggerlevelkiteonly.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_20371A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_20371A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1A891A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, d3forcel1disablekite.reg, triggerlevelkiteonly.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1A891A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1A891A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E006105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E006105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E006105B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E01F105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, smpsDynamic.reg, htAdhoc.reg, maxpowersave.reg, serializing.reg, d3forcel1disable1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E01F105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E01F105B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_663111AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, smpsDynamic.reg, htAdhoc.reg, maxpowersave.reg, serializing.reg, d3forcel1disablekite1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_663111AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_663111AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED.reg, customer0.reg, roamthreshA.reg, ignore11d.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED.reg, customer0.reg, roamthreshA.reg, ignore11d.reg, bandselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED1.reg, customer0.reg, roamthreshA.reg, ignore11d.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_4013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED1.reg, customer0.reg, roamthreshA.reg, ignore11d.reg, bandselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_4013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_4013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_5013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED2.reg, customer0.reg, roamthreshA.reg, ignore11d.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_5013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_5013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_6013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED2.reg, customer0.reg, roamthreshA.reg, ignore11d.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_6013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_6013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_0036.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer0LED1.reg, customer0_HB93.reg, roamthreshA.reg, ignore11d.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_0036.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_0036.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_0037.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer0LED1.reg, customer0_HB95.reg, roamthreshA.reg, ignore11d.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_0037.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_0037.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_F013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer1ani.reg, bandselect.reg, adhocchannelselect.reg, enableswretry, customer1roamPolicy.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_F013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_F013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_F013C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer1ani.reg, bandselect.reg, adhocchannelselect.reg, enableswretry, customer1roamPolicy.reg, minpower.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_F013C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_F013C.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_F01C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, customer1roamPolicy.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_F01C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_F01C.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_04221468.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer3.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_04221468.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_04221468.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E000105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer4b.reg, customer4a_ASPM.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = PciASPMOptIn, VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E000105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E000105B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E002105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer4b.reg, customer4a_ASPM.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = PciASPMOptIn, VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E002105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E002105B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_04281468.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer3a.reg, interruptpolling.reg, customer3_legacybgwmode.reg, adhocchannelselect.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_04281468.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_04281468.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_01051A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer3a.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_01051A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_01051A32.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_01121A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer3d.reg, d3hot.reg, adhocchannelselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_01121A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_01121A32.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_04061468.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer4.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_04061468.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_04061468.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_04231468.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer4a.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = PciASPMOptIn, VWiFiBus.CopyFiles

[ATHR_DEV_OS61_04231468.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_04231468.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E007105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer4a.reg, customer4adhoc.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = PciASPMOptIn, VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E007105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E007105B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S30A1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer4adhoc.reg, customer4a.reg, ratecap.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = PciASPMOptIn, VWiFiBus.CopyFiles

[ATHR_DEV_OS61_S30A1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S30A1.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_SS30A1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer4adhoc.reg, customer4as.reg, ratecap.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = PciASPMOptIn, VWiFiBus.CopyFiles

[ATHR_DEV_OS61_SS30A1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_SS30A1.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_0032168c.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer0_11n.reg, 5416.antennacontrols.reg, 5416.bgnxb.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_0032168c.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_0032168c.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_0033168c.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer0_11n.reg, 5416.antennacontrols.reg, 5416.bandselect.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_0033168c.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_0033168c.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_13C010CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.bandselect.reg, 5416.antennacontrols.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, customer1roamPolicy.reg, htAdhocdisable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_13C010CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_13C010CF.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_147C10CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.bandselect.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, smpsDynamic.reg, htAdhocdisable.reg, merlinshiftdelay.reg, d3forcel1disable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_147C10CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_147C10CF.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_147D10CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, htAdhocdisable.reg, merlinshiftdelay.reg, d3forcel1disable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_147D10CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_147D10CF.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_153710CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, htAdhocdisable.reg, d3forcel1disablekite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_153710CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_153710CF.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_7125144F.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.antennacontrols.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_7125144F.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_7125144F.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_03841014.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.antennacontrols.reg, xb72.via.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_03841014.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_03841014.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A171186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer5Led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A171186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A171186.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_10261A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cemspecled_func1_3.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_10261A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_10261A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_80111799.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer7Led.reg, ratecap.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_80111799.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_80111799.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer5.11nLED.reg, ratecap.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1186.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A691186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, pcibusconfig.reg, customer5.11nLED.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A691186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A691186.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A6D1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, pcibusconfig.reg, customer5.3x3.reg, customer5.11nLED.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A6D1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A6D1186.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A6F1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer5.PCIe11nLed.reg, expresscardaspmoff.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A6F1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A6F1186.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A701186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer5.3x3.reg, customer5.PCIe11nLed.reg, expresscardaspmoff.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A701186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A701186.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A7A1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, pcibusconfig.reg, customer5.11nLED.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A7A1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A7A1186.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A7B1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer5.11nLED.reg, ratecap.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A7B1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A7B1186.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_N2062.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, customer11.reg, customer11custom.reg, customer11_legacywmode.reg, cemspecled_func1_1.reg, customer11Ant.reg, rfKillDelayDetect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_N2062.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_N2062.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_N3072.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, customer11n.reg, customer11custom.reg, customer11_11nwmode.reg, cemspecled_func1_1.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_N3072.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_N3072.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_N3073.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, customer11n.reg, customer11custom.reg, customer11_11n40wmode.reg, cemspecled_func1_1.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_N3073.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_N3073.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S001A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_Samsung.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_S001A.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S001A.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S001B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_Samsung.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_S001B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S001B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S3067.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_Samsung.reg, rssiAdjust.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_S3067.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S3067.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S3067b.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_Samsung.reg, rssiAdjust.reg, cmdRegister.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_S3067b.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S3067b.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_10241A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htEnableWepTkip.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_10241A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_10241A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

;
; Vista Model section
;
[GIGA_DEV_E801.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E801.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_E811.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E811.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_E814.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E814.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_0013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_0013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_E901.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E901.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_E911.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E911.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_E912.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E912.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_E913.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer_GigaByteLed1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E913.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_E917.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer_GigaByteLed1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E917.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_E918.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer_GigaByteLed2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E918.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_E914.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer_GigaByte.reg, customer_GigaByteLed0.reg, 5416.antennacontrols.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E914.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_E916.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer_GigaByte.reg, customer_GigaByteLed1.reg, 5416.antennacontrols.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[GIGA_DEV_E916.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_0013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_0013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_001A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_001A.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_001B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_001B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_001C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_001C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_6313.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, cemspecled_func1_3.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_6313.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3064.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_3064.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1055.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, gpioled.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1055.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2055.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2055.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1030.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1030.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2030.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2030.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1031.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1031.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2031.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2031.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1041.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1041.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2041.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2041.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1042.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1042.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2042.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2042.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1051.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1051.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2051.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2051.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_7111144F.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, expresscardaspmoff.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_7111144F.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1052.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1052.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2052.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2052.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_01001A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer9Led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_01001A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1053.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1053.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2053.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2053.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1054.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1054.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2054.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2054.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1062.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1062.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2062.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2062.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1063.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1063.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2063.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2063.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1071.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_1071.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_90001385.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, expresscardaspmoff.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_90001385.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2A5F103C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer2.11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_2A5F103C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_11AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_11AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3072.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_3072.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_10671A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htWepTkipOpt.reg, htAdhoc.reg, indicaterxlinkspeed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_10671A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1A671A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, cemspecled_func1_1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_1A671A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_10711A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htEnableWepTkip.reg, htAdhoc.reg, d3forcel1disable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_10711A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1C711A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, 5416.bandselect.reg, htEnableWepTkip.reg, htAdhoc.reg, d3forcel1disable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_1C711A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_03011A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_03011A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3091.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_3091.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_008F106B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_008F106B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_309D17AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, Customer15a.led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_309D17AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_316417AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, Customer15b.led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_316417AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_7136144F.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, merlinshiftdelay.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_7136144F.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_D05B10FC.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, customer_IODATA.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_D05B10FC.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_T3091.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, smpsDynamic.reg, pcibusconfig.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_T3091.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_309917AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_309917AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_30A1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_30A1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_660311AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros11n.reg, htAdhoc.reg, cemspecled_func1_4.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_660311AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_30AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, htAdhoc.reg, triggerlevelkiteonly.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_30AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_30AB.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, htAdhoc.reg, janusda.reg, triggerlevelkiteonly.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_30AB.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_30A1a.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_30A1a.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_E023105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, htAdhoc.reg, cemspecled_func1_1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_E023105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_E029105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, cemspecled_func1_1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_E029105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_11121A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, cemspecled_func1_1.reg, d3forcel1disablekite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_11121A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_662111AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, cemspecled_func1_1.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_662111AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3091PB.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, pushbutton.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_3091PB.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1000168C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer2merlin.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_1000168C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1001168C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer2.11n.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_1001168C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3091SF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer_Samsung.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_3091SF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_03051A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, cemspecled_func1_1.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_03051A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_D8111113.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, cemspecled_func1_1.reg, htAdhoc.reg, d3forcel1disablekite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_D8111113.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_10891A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, cemspecled_func1_1.reg, htWepTkipOpt.reg, htAdhoc.reg, wirelessmodeselectkite.reg, triggerlevelkiteonly.reg, d3forcel1disablekite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_10891A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_20371A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, cemspecled_func1_1.reg, htEnableWepTkip.reg, htAdhoc.reg, wirelessmodeselectkite.reg, d3forcel1disablekite.reg, triggerlevelkiteonly.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_20371A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1A891A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, cemspecled_func1_1.reg, d3forcel1disablekite.reg, triggerlevelkiteonly.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_1A891A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_E006105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer3c.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_E006105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_E01F105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer3c.reg, smpsDynamic.reg, htAdhoc.reg, maxpowersave.reg, serializing.reg, d3forcel1disable1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_E01F105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_663111AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer3c.reg, smpsDynamic.reg, htAdhoc.reg, maxpowersave.reg, serializing.reg, d3forcel1disablekite1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_663111AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer0LED.reg, customer0.reg, roamthreshA.reg, ignore11d.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer0LED.reg, customer0.reg, roamthreshA.reg, ignore11d.reg, bandselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer0LED1.reg, customer0.reg, roamthreshA.reg, ignore11d.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_3013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_4013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer0LED1.reg, customer0.reg, roamthreshA.reg, ignore11d.reg, bandselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_4013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_5013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer0LED2.reg, customer0.reg, roamthreshA.reg, ignore11d.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_5013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_6013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer0LED2.reg, customer0.reg, roamthreshA.reg, ignore11d.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_6013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_0036.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer0LED1.reg, customer0_HB93.reg, roamthreshA.reg, ignore11d.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_0036.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_0037.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer0LED1.reg, customer0_HB95.reg, roamthreshA.reg, ignore11d.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_0037.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_F013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer1ani.reg, bandselect.reg, adhocchannelselect.reg, enableswretry, customer1roamPolicy.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_F013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_F013C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer1ani.reg, bandselect.reg, adhocchannelselect.reg, enableswretry, customer1roamPolicy.reg, minpower.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_F013C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_F01C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, customer1roamPolicy.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_F01C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_04221468.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer3.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_04221468.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_E000105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer4b.reg, customer4a_ASPM.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf
Needs           = PciASPMOptIn

[ATHR_DEV_E000105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_E002105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer4b.reg, customer4a_ASPM.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf
Needs           = PciASPMOptIn

[ATHR_DEV_E002105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_04281468.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer3a.reg, interruptpolling.reg, customer3_legacybgwmode.reg, adhocchannelselect.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_04281468.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_01051A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer3a.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_01051A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_01121A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer3d.reg, d3hot.reg, adhocchannelselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_01121A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_04061468.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer4.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_04061468.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_04231468.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer4a.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf
Needs           = PciASPMOptIn

[ATHR_DEV_04231468.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_E007105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer4a.reg, customer4adhoc.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf
Needs           = PciASPMOptIn

[ATHR_DEV_E007105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_S30A1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, htAdhoc.reg, customer4adhoc.reg, customer4a.reg, ratecap.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = machine.inf
Needs           = PciASPMOptIn

[ATHR_DEV_S30A1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_SS30A1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, htAdhoc.reg, customer4adhoc.reg, customer4as.reg, ratecap.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = machine.inf
Needs           = PciASPMOptIn

[ATHR_DEV_SS30A1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_0032168c.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer0_11n.reg, 5416.antennacontrols.reg, 5416.bgnxb.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_0032168c.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_0033168c.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer0_11n.reg, 5416.antennacontrols.reg, 5416.bandselect.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_0033168c.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_13C010CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, 5416.bandselect.reg, 5416.antennacontrols.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, customer1roamPolicy.reg, htAdhocdisable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_13C010CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_147C10CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, 5416.bandselect.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, smpsDynamic.reg, htAdhocdisable.reg, merlinshiftdelay.reg, d3forcel1disable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_147C10CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_147D10CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, htAdhocdisable.reg, merlinshiftdelay.reg, d3forcel1disable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_147D10CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_153710CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, htAdhocdisable.reg, d3forcel1disablekite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_153710CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_7125144F.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, 5416.antennacontrols.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_7125144F.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_03841014.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, 5416.antennacontrols.reg, xb72.via.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_03841014.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3A171186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer5Led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_3A171186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_10261A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, cemspecled_func1_3.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_10261A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_80111799.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer7Led.reg, ratecap.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_80111799.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer5.11nLED.reg, ratecap.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3A691186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, pcibusconfig.reg, customer5.11nLED.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_3A691186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3A6D1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, pcibusconfig.reg, customer5.3x3.reg, customer5.11nLED.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_3A6D1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3A6F1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer5.PCIe11nLed.reg, expresscardaspmoff.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_3A6F1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3A701186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer5.3x3.reg, customer5.PCIe11nLed.reg, expresscardaspmoff.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_3A701186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3A7A1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, pcibusconfig.reg, customer5.11nLED.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_3A7A1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3A7B1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, customer5.11nLED.reg, ratecap.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_3A7B1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_N2062.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, customer11.reg, customer11custom.reg, customer11_legacywmode.reg, cemspecled_func1_1.reg, customer11Ant.reg, rfKillDelayDetect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_N2062.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_N3072.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, customer11n.reg, customer11custom.reg, customer11_11nwmode.reg, cemspecled_func1_1.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_N3072.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_N3073.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, customer11n.reg, customer11custom.reg, customer11_11n40wmode.reg, cemspecled_func1_1.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_N3073.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_S001A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer_Samsung.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_S001A.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_S001B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer_Samsung.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_S001B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_S3067.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer_Samsung.reg, rssiAdjust.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_S3067.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_S3067b.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros.reg, customer_Samsung.reg, rssiAdjust.reg, cmdRegister.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_S3067b.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_10241A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg, atheros11n.reg, cemspecled_func1_1.reg, htEnableWepTkip.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_10241A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

;;End of Others Section

[atheros_os61.reg]
HKR, Ndi,                           Service,    0, "athr"
HKR, Ndi\Interfaces,                UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,                LowerRange, 0, "wlan,ethernet,vwifi"

[atheros_os60.reg]
HKR, Ndi,                           Service,    0, "athr"
HKR, Ndi\Interfaces,                UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,                LowerRange, 0, "wlan,ethernet"

[atheros11n.reg]
HKR, Ndi\params\*ReceiveBuffers,    ParamDesc,  0, "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,    default,    0, "256"
HKR, Ndi\params\*ReceiveBuffers,    min,        0, "1"
HKR, Ndi\params\*ReceiveBuffers,    max,        0, "00000512"
HKR, Ndi\params\*ReceiveBuffers,    step,       0, "1"
HKR, Ndi\params\*ReceiveBuffers,    Base,       0, "10"
HKR, Ndi\params\*ReceiveBuffers,    type,       0, "int"
HKR, Ndi\params\*TransmitBuffers,   ParamDesc,  0, "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,   default,    0, "512"
HKR, Ndi\params\*TransmitBuffers,   min,        0, "1"
HKR, Ndi\params\*TransmitBuffers,   max,        0, "00000512"
HKR, Ndi\params\*TransmitBuffers,   step,       0, "1"
HKR, Ndi\params\*TransmitBuffers,   Base,       0, "10"
HKR, Ndi\params\*TransmitBuffers,   type,       0, "int"
HKR, Ndi\params\NetworkAddress,     ParamDesc,  0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,     default,    0,  ""
HKR, Ndi\params\NetworkAddress,     LimitText,  0,  "12"
HKR, Ndi\params\NetworkAddress,     UpperCase,  0,  "1"
HKR, Ndi\params\NetworkAddress,     optional,   0,  "1"
HKR, Ndi\params\NetworkAddress,     type,       0,  "edit"
HKR, Ndi\params\shortPreamble,      ParamDesc,  0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,      Base,       0,  "10"
HKR, Ndi\params\shortPreamble,      default,    0,  "1"
HKR, Ndi\params\shortPreamble,      type,       0,  "enum"
HKR, Ndi\params\shortPreamble\enum, "1",        0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0",        0,  %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid,      ParamDesc,  0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,      default,    0,  "60"
HKR, Ndi\params\scanTimeValid,      min,        0,  "20"
HKR, Ndi\params\scanTimeValid,      max,        0,  "120"
HKR, Ndi\params\scanTimeValid,      step,       0,  "5"
HKR, Ndi\params\scanTimeValid,      base,       0,  "10"
HKR, Ndi\params\scanTimeValid,      type,       0,  "int"

;/* Enable these if VLAN or 802.1p is to be enabled */
;HKR, Ndi\Params\*PriorityVLANTag,  ParamDesc,  , %PriorityVLAN%
;HKR, Ndi\Params\*PriorityVLANTag,  default,    , "3"
;HKR, Ndi\Params\*PriorityVLANTag,  type,       , "enum"
;HKR, Ndi\Params\*PriorityVLANTag\enum, 0,      , %PriorityVLANDisabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 1,      , %PriorityEnabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 2,      , %VLANEnabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 3,      , %PriorityVLANEnabled%

[atheros.reg]
HKR, Ndi\params\*ReceiveBuffers,    ParamDesc,  0, "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,    default,    0, "256"
HKR, Ndi\params\*ReceiveBuffers,    min,        0, "1"
HKR, Ndi\params\*ReceiveBuffers,    max,        0, "00000512"
HKR, Ndi\params\*ReceiveBuffers,    step,       0, "1"
HKR, Ndi\params\*ReceiveBuffers,    Base,       0, "10"
HKR, Ndi\params\*ReceiveBuffers,    type,       0, "int"
HKR, Ndi\params\*TransmitBuffers,   ParamDesc,  0, "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,   default,    0, "256"
HKR, Ndi\params\*TransmitBuffers,   min,        0, "1"
HKR, Ndi\params\*TransmitBuffers,   max,        0, "00000512"
HKR, Ndi\params\*TransmitBuffers,   step,       0, "1"
HKR, Ndi\params\*TransmitBuffers,   Base,       0, "10"
HKR, Ndi\params\*TransmitBuffers,   type,       0, "int"
HKR, Ndi\params\NetworkAddress,     ParamDesc,  0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,     default,    0,  ""
HKR, Ndi\params\NetworkAddress,     LimitText,  0,  "12"
HKR, Ndi\params\NetworkAddress,     UpperCase,  0,  "1"
HKR, Ndi\params\NetworkAddress,     optional,   0,  "1"
HKR, Ndi\params\NetworkAddress,     type,       0,  "edit"
HKR, Ndi\params\shortPreamble,      ParamDesc,  0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,      Base,       0,  "10"
HKR, Ndi\params\shortPreamble,      default,    0,  "1"
HKR, Ndi\params\shortPreamble,      type,       0,  "enum"
HKR, Ndi\params\shortPreamble\enum, "1",        0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0",        0,  %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid,      ParamDesc,  0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,      default,    0,  "60"
HKR, Ndi\params\scanTimeValid,      min,        0,  "20"
HKR, Ndi\params\scanTimeValid,      max,        0,  "120"
HKR, Ndi\params\scanTimeValid,      step,       0,  "5"
HKR, Ndi\params\scanTimeValid,      base,       0,  "10"
HKR, Ndi\params\scanTimeValid,      type,       0,  "int"

[atheros.DelReg]
HKR,,NetBand
HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
HKR,Ndi\Params\tpc
HKR,,tpc
HKR,Ndi\Params\authTypeUseOnly
HKR,,authTypeUseOnly
HKR,,AdHocBand
HKR,,AwakeTimePerf
HKR,,beaconInterval
HKR,,bkScanEnable
HKR,,bssType
HKR,,ccode
HKR,,clist
HKR,,defaultKey
HKR,,EncryptionAlg
HKR,,FragThreshold
HKR,,HwTxRetries
HKR,,privacyInvoked
HKR,,QoS
HKR,,rateCtrlEnable
HKR,,RTSThreshold
HKR,,scanType
HKR,,SwTxRetryScale
HKR,,SmeEnable
HKR,,aifs
HKR,,cwmin
HKR,,halPcieClockReq
HKR,Ndi\params,MapRegisters,0x2000
HKR,,MapRegisters
HKR,Ndi\params,radioEnable,0x2000
HKR,Ndi\params,sleepMode,0x2000
HKR,,sleepMode
HKR,,gpioFunc0ActHi
HKR,,gpioFunc1ActHi
HKR,,gpioLedCustom
HKR,,gpioPinFunc0
HKR,,gpioPinFunc1
HKR,,transmitRateMax
HKR, Ndi\params\*TransmitBuffers
HKR,,*TransmitBuffers
HKR,,rxChainMask
HKR,,txChainMaskLegacy
HKR,,rxChainMaskLegacy
HKR,,rxChainDetect
HKR,,rxChainDetectRef
HKR,,rxChainDetectThreshA
HKR,,rxChainDetectThreshG
HKR,,rxChainDetectDeltaA
HKR,,rxChainDetectDeltaG
HKR, Ndi\params\smpsDynamic
HKR,,d3forcel1disable.reg
HKR,,d3forcel1disablekite.reg
HKR,,wmeEnabled
HKR,,halPcieWaen

;;Customized Section

[expresscardaspmoff.reg]
HKR, ,                                  pciDetectEnable,                0x00002,  "2"
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1"
HKR, ,                                  pcieAspm,                       0x00002,  "0"

[rfKillDelayDetect.reg]
HKR, ,                                  rfKillDelayDetect,              0x00002,  "1"

[d3hot.reg] 
HKR, ,                                  halPciePowerReset,              0x00002,  "0"
HKR, ,                                  halPcieRestore,                 0x00002,  "1"

[enableswretry] 
HKR, ,                                  numSwRetries,                   0x00002,  "4"

[interruptpolling.reg]
HKR, ,                                  isrPollInterval,                0x00002,  "100"

[pcibusconfig.reg]
HKR, ,                                  BusConfig,                 	0x00002,  "0"
HKR, ,                                  serializeRegMode,               0x00002,  "2"

[serializing.reg]
HKR, ,                                  serializeRegMode,               0x00002,  "1"

[bandselect.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,        %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,        "10"
HKR, Ndi\params\NetBand,                default,                        0,        "1647"
HKR, Ndi\params\NetBand,                type,                           0,        "enum"
HKR, Ndi\params\NetBand\enum,           "1647",                         0,        %Auto%
HKR, Ndi\params\NetBand\enum,           "1603",                         0,        %5GOnly%
HKR, Ndi\params\NetBand\enum,           "44",                           0,        %2GOnly%

[roamthreshA.reg]
HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,        %roamRssiA%
HKR, Ndi\params\roamRssiA,              default,                        0,        "15"
HKR, Ndi\params\roamRssiA,              min,                            0,        "1"
HKR, Ndi\params\roamRssiA,              max,                            0,        "95"
HKR, Ndi\params\roamRssiA,              step,                           0,        "1"
HKR, Ndi\params\roamRssiA,              base,                           0,        "10"
HKR, Ndi\params\roamRssiA,              type,                           0,        "int"

[ignore11d.reg]
HKR,NDI\params\ignore11dBeacon,         ParamDesc,,                               %11DModeSwitch%
HKR,NDI\params\ignore11dBeacon,         type,,                                    "enum"
HKR,NDI\params\ignore11dBeacon,         Default,,                                 "1"
HKR,NDI\params\ignore11dBeacon\enum,    0,,                                       %Enable%
HKR,NDI\params\ignore11dBeacon\enum,    1,,                                       %Disable%

;[radioswitch.reg]
;HKR, Ndi\params\radioEnable,            ParamDesc,                      0,        %radioEnable%
;HKR, Ndi\params\radioEnable,            Base,                           0,        "10"
;HKR, Ndi\params\radioEnable,            default,                        0,        "1"
;HKR, Ndi\params\radioEnable,            type,                           0,        "enum"
;HKR, Ndi\params\radioEnable\enum,       "1",                            0,        %radioEnableOn%
;HKR, Ndi\params\radioEnable\enum,       "0",                            0,        %radioEnableOff%

[overridetxok.reg]
HKR, ,                                  OverrideTxOk,                   0x00002,  "1"

[adhocchannelselect.reg]
HKR, Ndi\params\defaultIbssChannel,     ParamDesc,                      0,        %adhocchannel%
HKR, Ndi\params\defaultIbssChannel,     default,                        0,        "10"
HKR, Ndi\params\defaultIbssChannel,     min,                            0,        "1"
HKR, Ndi\params\defaultIbssChannel,     max,                            0,        "11"
HKR, Ndi\params\defaultIbssChannel,     step,                           0,        "1"
HKR, Ndi\params\defaultIbssChannel,     base,                           0,        "10"
HKR, Ndi\params\defaultIbssChannel,     type,                           0,        "int"

[5416.bgnxb.reg]
HKR, ,                                  NetBand,                        0x00002,  "26636"
HKR, ,                                  wmodeselect,                    0x00002,  "26636"

[5416.bandselect.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "130671"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "130671",                       0,  %Auto%
HKR, Ndi\params\NetBand\enum,           "104003",                       0,  %5GOnly%
HKR, Ndi\params\NetBand\enum,           "26668",                        0,  %2GOnly%

[wirelessmodeselectkite.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "26636"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "26636",                        0,  %WirelessModeAuto%
HKR, Ndi\params\NetBand\enum,           "12",                           0,  %WirelessMode11bgOnly%

[5416.antennacontrols.reg] 
HKR, ,                                  rxChainMask,                 	0x00002,  "7"
;HKR, ,                                  txChainMaskLegacy,              0x00002,  "5"
HKR, ,                                  rxChainMaskLegacy,           	0x00002,  "7"
HKR, ,                                  rxChainDetect,                  0x00002,  "1"
HKR, ,                                  rxChainDetectRef,               0x00002,  "0"
HKR, ,                                  rxChainDetectThreshA,           0x00002,  "0"
HKR, ,                                  rxChainDetectThreshG,           0x00002,  "0"
HKR, ,                                  rxChainDetectDeltaA,            0x00002,  "20"
HKR, ,                                  rxChainDetectDeltaG,            0x00002,  "20"

[pushbutton.reg]
HKR, ,                                  wpsButtonGpio,                  0x00002,  "9"

[smpsDynamic.reg]
HKR, Ndi\params\smpsDynamic,            ParamDesc,  0,  %smpsDynamic%
HKR, Ndi\params\smpsDynamic,            Base,       0,  "10"
HKR, Ndi\params\smpsDynamic,            default,    0,  "0"
HKR, Ndi\params\smpsDynamic,            type,       0,  "enum"
HKR, Ndi\params\smpsDynamic\enum,       "1",        0,  %Enable%
HKR, Ndi\params\smpsDynamic\enum,       "0",        0,  %Disable%

[customer0.reg]
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR, ,                                  scanTimePreSleep,               0x00002,  "60" 
HKR, ,                                  capLinkSp,                      0x00002,  "1" 
HKR, ,                                  pcieAspm,                       0x00002,  "2" 
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1" 
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,        %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,        "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,        "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,        "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,        "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,        "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,        "int"

[customer0_HB95.reg]
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR, ,                                  scanTimePreSleep,               0x00002,  "60" 
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,        %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,        "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,        "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,        "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,        "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,        "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,        "int"

[customer0_HB93.reg]
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR, ,                                  scanTimePreSleep,               0x00002,  "60" 
HKR, ,                                  pcieAspm,                       0x00002,  "2" 
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1" 
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,        %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,        "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,        "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,        "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,        "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,        "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,        "int"

[customer0LED.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "0"

[customer0LED1.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  halPcieClockReq,                0x00002,  "0"

[customer0LED2.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  halPcieClockReq,                0x00002,  "0"

[customer0_11n.reg]
;PCIe Related
HKR, ,                                  radioEnableInterval,            0x00002,  "5"
HKR, ,                                  pcieAspm,                 	0x00002,  "2"
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  forceWake,                 	0x00002,  "0"
HKR, ,                                  antennaSwitchSwap,              0x00002,  "1"
;LED Related
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
;General Customer0
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR,NDI\params\ignore11dBeacon,ParamDesc,,	%11DModeSwitch%
HKR,NDI\params\ignore11dBeacon,type,,		"enum"
HKR,NDI\params\ignore11dBeacon,Default,,	"1"
HKR,NDI\params\ignore11dBeacon\enum,0,,		%Enable%
HKR,NDI\params\ignore11dBeacon\enum,1,,		%Disable%

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,  %roamRssiA%
HKR, Ndi\params\roamRssiA,              default,                        0,  "15"
HKR, Ndi\params\roamRssiA,              min,                            0,  "1"
HKR, Ndi\params\roamRssiA,              max,                            0,  "95"
HKR, Ndi\params\roamRssiA,           	step,                           0,  "1"
HKR, Ndi\params\roamRssiA,           	base,                           0,  "10"
HKR, Ndi\params\roamRssiA,           	type,                           0,  "int"

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

[customer1ani.reg]
HKR, Ndi\params\rssiThrHigh,            ParamDesc,                      0,        %rssiThrHigh%
HKR, Ndi\params\rssiThrHigh,            Base,                           0,        "10"
HKR, Ndi\params\rssiThrHigh,            default,                        0,        "40"
HKR, Ndi\params\rssiThrHigh,            type,                           0,        "enum"
HKR, Ndi\params\rssiThrHigh\enum,       "40",                           0,        %rssiThrHighNormal%
HKR, Ndi\params\rssiThrHigh\enum,       "32",                           0,        %rssiThrHighMin%

[customer1roamPolicy.reg]
HKR, Ndi\params\roamPolicy,             ParamDesc,                      0,        %roamPolicy%
HKR, Ndi\params\roamPolicy,             Base,                           0,        "10"
HKR, Ndi\params\roamPolicy,             default,                        0,        "3"
HKR, Ndi\params\roamPolicy,             type,                           0,        "enum"
HKR, Ndi\params\roamPolicy\enum,        "1",                            0,        %roamPolicyVeryLow%
HKR, Ndi\params\roamPolicy\enum,        "2",                            0,        %roamPolicyLow%
HKR, Ndi\params\roamPolicy\enum,        "3",                            0,        %roamPolicyNormal%
HKR, Ndi\params\roamPolicy\enum,        "4",                            0,        %roamPolicyHigh%
HKR, Ndi\params\roamPolicy\enum,        "5",                            0,        %roamPolicyVeryHigh%

[customer2.reg]
HKR,,                                   linkLEDFunc,                    0,        "53"
HKR,,                                   activityLEDFunc,                0,        "51"
HKR,,                                   connectionLEDFunc,              0,        "55"

[customer2.11n.reg]
HKR, ,					gpioPinFunc0,        		0x00002,  "1"

[customer2merlin.reg]
HKR, ,					gpioPinFunc0,        		0x00002,  "1"
HKR, ,					gpioFunc0ActHi,        		0x00002,  "1"

[customer3.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  LinkLEDFunc,                    0x00002,  "19"
HKR, ,                                  ActivityLEDFunc,                0x00002,  "21"

[customer3a.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

;[customer3b.reg]
;HKR, ,                                  gpioPinFunc1,			0x00002,  "3"
;HKR, ,                                  overrideACstatus,		0x00002,  "1"
;HKR, ,                                  halPcieClockReq,		0x00002,  "0"
;HKR, ,                                  gpioLedCustom,			0x00002,  "4"
;HKR, ,                                  gpioFunc1ActHi,		0x00002,  "0"

[customer3c.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

[customer3d.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "0"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

[customer3_legacybgwmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "12"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "4",                            0,        %wModeLegacy11bonly%
HKR, Ndi\params\wModeSelect\enum,       "12",                           0,        %wModeLegacy11bg%

[customer4.reg]
HKR, ,					gpioPinFunc0,        		0x00002,  "1"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4a.reg]
HKR, ,                                  gpioPinFunc0,        		0x00002,  "1"
HKR, ,                                  gpioFunc0ActHi,      		0x00002,  "0"
HKR, ,                                  halPcieClockReq,        	0x00002,  "0"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4as.reg]
HKR, ,                                  gpioPinFunc0,        		0x00002,  "8"
HKR, ,                                  gpioFunc0ActHi,      		0x00002,  "0"
HKR, ,                                  halPcieClockReq,        	0x00002,  "0"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4adhoc.reg]
HKR, ,                                  defaultIbssChannel,             0x00002,  "11"

[customer4b.reg]
HKR, ,					gpioPinFunc0,        		0x00002,  "3"
HKR, ,					gpioFunc0ActHi,      		0x00002,  "0"
HKR, ,					halPcieClockReq,        	0x00002,  "0"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4a_ASPM.reg]
HKR, ,                                  pcieAspm,                       0x00002,  "0"

[customer5Led.reg]
HKR, ,                                  softLEDEnable,                  0x00002,  "1"
HKR, ,                                  swapDefaultLED,                 0x00002,  "1"

[customer5.11nLED.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "1"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "2"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

[customer5.PCIe11nLed.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"

[customer5.3x3.reg]
HKR, ,                                  txChainMask,                 	0x00002,  "7"
HKR, ,                                  rxChainMask,                 	0x00002,  "7"

[customer7Led.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "2"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "2"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "1"

[customer9Led.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"

[Customer15a.led.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[Customer15b.led.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[gpioled.reg]
HKR,,                                   linkLEDFunc,                    0,        "49"
HKR,,                                   activityLEDFunc,                0,        "51"
HKR,,                                   connectionLEDFunc,              0,        "55"

[ratecap.reg]
HKR, ,                                  txCoalescingEnable,             0x00002,  "1"

[customer11n.reg]
HKR, Ndi\params\*ReceiveBuffers,        ParamDesc,                      0,        "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,        default,                        0,        "256"
HKR, Ndi\params\*ReceiveBuffers,        min,                            0,        "1"
HKR, Ndi\params\*ReceiveBuffers,        max,                            0,        "00000512"
HKR, Ndi\params\*ReceiveBuffers,        step,                           0,        "1"
HKR, Ndi\params\*ReceiveBuffers,        Base,                           0,        "10"
HKR, Ndi\params\*ReceiveBuffers,        type,                           0,        "int"
HKR, Ndi\params\*TransmitBuffers,       ParamDesc,                      0,        "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,       default,                        0,        "512"
HKR, Ndi\params\*TransmitBuffers,       min,                            0,        "1"
HKR, Ndi\params\*TransmitBuffers,       max,                            0,        "00000512"
HKR, Ndi\params\*TransmitBuffers,       step,                           0,        "1"
HKR, Ndi\params\*TransmitBuffers,       Base,                           0,        "10"
HKR, Ndi\params\*TransmitBuffers,       type,                           0,        "int"
HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,        %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,        "10"
HKR, Ndi\params\shortPreamble,          default,                        0,        "1"
HKR, Ndi\params\shortPreamble,          type,                           0,        "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,        %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,        %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,        %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          default,                        0,        "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,        "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,        "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,        "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,        "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,        "int"

[customer11.reg]
HKR, Ndi\params\*ReceiveBuffers,    ParamDesc,  0, "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,    default,    0, "256"
HKR, Ndi\params\*ReceiveBuffers,    min,        0, "1"
HKR, Ndi\params\*ReceiveBuffers,    max,        0, "00000512"
HKR, Ndi\params\*ReceiveBuffers,    step,       0, "1"
HKR, Ndi\params\*ReceiveBuffers,    Base,       0, "10"
HKR, Ndi\params\*ReceiveBuffers,    type,       0, "int"
HKR, Ndi\params\*TransmitBuffers,   ParamDesc,  0, "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,   default,    0, "256"
HKR, Ndi\params\*TransmitBuffers,   min,        0, "1"
HKR, Ndi\params\*TransmitBuffers,   max,        0, "00000512"
HKR, Ndi\params\*TransmitBuffers,   step,       0, "1"
HKR, Ndi\params\*TransmitBuffers,   Base,       0, "10"
HKR, Ndi\params\*TransmitBuffers,   type,       0, "int"
HKR, Ndi\params\shortPreamble,      ParamDesc,  0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,      Base,       0,  "10"
HKR, Ndi\params\shortPreamble,      default,    0,  "1"
HKR, Ndi\params\shortPreamble,      type,       0,  "enum"
HKR, Ndi\params\shortPreamble\enum, "1",        0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0",        0,  %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid,      ParamDesc,  0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,      default,    0,  "60"
HKR, Ndi\params\scanTimeValid,      min,        0,  "20"
HKR, Ndi\params\scanTimeValid,      max,        0,  "120"
HKR, Ndi\params\scanTimeValid,      step,       0,  "5"
HKR, Ndi\params\scanTimeValid,      base,       0,  "10"
HKR, Ndi\params\scanTimeValid,      type,       0,  "int"

[customer11custom.reg]
HKR, Ndi\params\bkScanEnable,           ParamDesc,                      0,        %bkScanEnable%
HKR, Ndi\params\bkScanEnable,           Base,                           0,        "10"
HKR, Ndi\params\bkScanEnable,           default,                        0,        "1"
HKR, Ndi\params\bkScanEnable,           type,                           0,        "enum"
HKR, Ndi\params\bkScanEnable\enum,      "1",                            0,        %bkScanEnableOn%
HKR, Ndi\params\bkScanEnable\enum,      "0",                            0,        %bkScanEnableOff%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,        %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,        "10"
HKR, Ndi\params\radioEnable,            default,                        0,        "1"
HKR, Ndi\params\radioEnable,            type,                           0,        "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,        %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,        %radioEnableOff%

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,        %roamRssi11A%
HKR, Ndi\params\roamRssiA,              default,                        0,        "15"
HKR, Ndi\params\roamRssiA,              min,                            0,        "1"
HKR, Ndi\params\roamRssiA,              max,                            0,        "95"
HKR, Ndi\params\roamRssiA,              step,                           0,        "1"
HKR, Ndi\params\roamRssiA,              base,                           0,        "10"
HKR, Ndi\params\roamRssiA,              type,                           0,        "int"

HKR, Ndi\params\roamRssiBOnly,          ParamDesc,                      0,        %roamRssi11BOnly%
HKR, Ndi\params\roamRssiBOnly,          default,                        0,        "8"
HKR, Ndi\params\roamRssiBOnly,          min,                            0,        "0"
HKR, Ndi\params\roamRssiBOnly,          max,                            0,        "95"
HKR, Ndi\params\roamRssiBOnly,          step,                           0,        "1"
HKR, Ndi\params\roamRssiBOnly,          base,                           0,        "10"
HKR, Ndi\params\roamRssiBOnly,          type,                           0,        "int"

HKR, Ndi\params\roamRssiB,              ParamDesc,                      0,        %roamRssi11B%
HKR, Ndi\params\roamRssiB,              default,                        0,        "24"
HKR, Ndi\params\roamRssiB,              min,                            0,        "0"
HKR, Ndi\params\roamRssiB,              max,                            0,        "95"
HKR, Ndi\params\roamRssiB,              step,                           0,        "1"
HKR, Ndi\params\roamRssiB,              base,                           0,        "10"
HKR, Ndi\params\roamRssiB,              type,                           0,        "int"

HKR, Ndi\params\roamRateA,              ParamDesc,                      0,        %roamRateA%
HKR, Ndi\params\roamRateA,              Base,                           0,        "10"
HKR, Ndi\params\roamRateA,              default,                        0,        "24000"
HKR, Ndi\params\roamRateA,              type,                           0,        "enum"
HKR, Ndi\params\roamRateA\enum,         "6000",                         0,        %roamRateA6M%
HKR, Ndi\params\roamRateA\enum,         "9000",                         0,        %roamRateA9M%
HKR, Ndi\params\roamRateA\enum,         "12000",                        0,        %roamRateA12M%
HKR, Ndi\params\roamRateA\enum,         "18000",                        0,        %roamRateA18M%
HKR, Ndi\params\roamRateA\enum,         "24000",                        0,        %roamRateA24M%
HKR, Ndi\params\roamRateA\enum,         "36000",                        0,        %roamRateA36M%
HKR, Ndi\params\roamRateA\enum,         "48000",                        0,        %roamRateA48M%
HKR, Ndi\params\roamRateA\enum,         "54000",                        0,        %roamRateA54M%

HKR, Ndi\params\roamRateBOnly,          ParamDesc,                      0,        %roamRateBOnly%
HKR, Ndi\params\roamRateBOnly,          Base,                           0,        "10"
HKR, Ndi\params\roamRateBOnly,          default,                        0,        "5000"
HKR, Ndi\params\roamRateBOnly,          type,                           0,        "enum"
HKR, Ndi\params\roamRateBOnly\enum,     "1000",                         0,        %roamRateBOnly1M%
HKR, Ndi\params\roamRateBOnly\enum,     "2000",                         0,        %roamRateBOnly2M%
HKR, Ndi\params\roamRateBOnly\enum,     "5000",                         0,        %roamRateBOnly5M%
HKR, Ndi\params\roamRateBOnly\enum,     "11000",                        0,        %roamRateBOnly11M%

HKR, Ndi\params\roamRateB,              ParamDesc,                      0,        %roamRateB%
HKR, Ndi\params\roamRateB,              Base,                           0,        "10"
HKR, Ndi\params\roamRateB,              default,                        0,        "9000"
HKR, Ndi\params\roamRateB,              type,                           0,        "enum"
HKR, Ndi\params\roamRateB\enum,         "1000",                         0,        %roamRateB1M%
HKR, Ndi\params\roamRateB\enum,         "2000",                         0,        %roamRateB2M%
HKR, Ndi\params\roamRateB\enum,         "5000",                         0,        %roamRateB5M%
HKR, Ndi\params\roamRateB\enum,         "6000",                         0,        %roamRateB6M%
HKR, Ndi\params\roamRateB\enum,         "9000",                         0,        %roamRateB9M%
HKR, Ndi\params\roamRateB\enum,         "11000",                        0,        %roamRateB11M%

HKR, Ndi\params\pcieAspm,               ParamDesc,                      0,        %pcieAspm%
HKR, Ndi\params\pcieAspm,               Base,                           0,        "10"
HKR, Ndi\params\pcieAspm,               default,                        0,        "0"
HKR, Ndi\params\pcieAspm,               type,                           0,        "enum"
HKR, Ndi\params\pcieAspm\enum,          "0",                            0,        %pcieAspmOff%
HKR, Ndi\params\pcieAspm\enum,          "1",                            0,        %pcieAspmL0sOn%
HKR, Ndi\params\pcieAspm\enum,          "2",                            0,        %pcieAspmL1On%
HKR, Ndi\params\pcieAspm\enum,          "3",                            0,        %pcieAspmL0sandL1On%

[customer11_11n40wmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "129055"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "26628",                        0,        %wModeSelect11bonly%
HKR, Ndi\params\wModeSelect\enum,       "102403",                       0,        %wModeSelect11na%
HKR, Ndi\params\wModeSelect\enum,       "26652",                        0,        %wModeSelect11nbg%
HKR, Ndi\params\wModeSelect\enum,       "129055",                       0,        %wModeSelect11abgn%

[customer11_11nwmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "6175"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "2052",                         0,        %wModeSelect11bonly%
HKR, Ndi\params\wModeSelect\enum,       "4099",                         0,        %wModeSelect11na%
HKR, Ndi\params\wModeSelect\enum,       "2076",                         0,        %wModeSelect11nbg%
HKR, Ndi\params\wModeSelect\enum,       "6175",                         0,        %wModeSelect11abgn%

[customer11_legacywmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "31"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "4",                            0,        %wModeLegacy11bonly%
HKR, Ndi\params\wModeSelect\enum,       "3",                            0,        %wModeLegacy11a%
HKR, Ndi\params\wModeSelect\enum,       "28",                           0,        %wModeLegacy11bg%
HKR, Ndi\params\wModeSelect\enum,       "31",                           0,        %wModeLegacy11abg%

[customer11Ant.reg]
HKR, Ndi\params\antennaSwitch,          ParamDesc,                      0,        %antennaSwitch%
HKR, Ndi\params\antennaSwitch,          Base,                           0,        "10"
HKR, Ndi\params\antennaSwitch,          default,                        0,        "2"
HKR, Ndi\params\antennaSwitch,          type,                           0,        "enum"
HKR, Ndi\params\antennaSwitch\enum,     "0",                            0,        %antennaSwitchA%
HKR, Ndi\params\antennaSwitch\enum,     "1",                            0,        %antennaSwitchB%
HKR, Ndi\params\antennaSwitch\enum,     "2",                            0,        %antennaSwitchAuto%

[customer_GigaByte.reg]
HKR, ,                          txChainMask,          0x00002,  "5"

[customer_GigaByteLed0.reg]
HKR, ,                  		LinkLedFunc,       		0, "19"
HKR, ,                  		ActivityLedFunc,       	0, "21" 

[customer_GigaByteLed1.reg]
HKR, ,                  		LinkLedFunc,       		0, "03"
HKR, ,                  		ActivityLedFunc,       		0, "05"

[customer_GigaByteLed2.reg]
HKR, ,                  		LinkLedFunc,       		0, "07"
HKR, ,                  		ActivityLedFunc,       		0, "05"

[customer_Samsung.reg]
HKR, Ndi\params\sleepMode,                ParamDesc,                      0,  %PowerSaveMode%
HKR, Ndi\params\sleepMode,                Base,                           0,  "10"
HKR, Ndi\params\sleepMode,                default,                        0,  "2"
HKR, Ndi\params\sleepMode,                type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,           "0",                            0,  %Off%
HKR, Ndi\params\sleepMode\enum,           "1",                            0,  %Maximum%
HKR, Ndi\params\sleepMode\enum,           "2",                            0,  %Normal%
HKR, NDI\params\ignore11dBeacon,ParamDesc,,	%802_11d%
HKR, NDI\params\ignore11dBeacon,type,,		"enum"
HKR, NDI\params\ignore11dBeacon,Default,,	"1"
HKR, NDI\params\ignore11dBeacon\enum,0,,	%Enable%
HKR, NDI\params\ignore11dBeacon\enum,1,,	%Disable%
HKR, ,                                  pcieAspm,                       0x00002,  "2" 
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1" 

[xb72.via.reg]
HKLM, SYSTEM\CurrentControlSet\Services\pci\Parameters,168c0024,0x00000001, 00,00,00,20,00,00,00,00

[rssiAdjust.reg]
HKR, ,                                  rssiAdjust,                     0x00002,  "7"

[cmdRegister.reg]
HKR, ,                                  cmdRegister.reg,                0x00002,  "838"

[htAdhocdisable.reg]
HKR, ,                                  htAdhocEnable,                  0x00002,  "0"

[htAdhoc.reg]
HKR, NDI\params\htAdhocEnable,ParamDesc,,	%AdHoc11n%
HKR, NDI\params\htAdhocEnable,type,,		"enum"
HKR, NDI\params\htAdhocEnable,Default,,	        "0"
HKR, NDI\params\htAdhocEnable\enum,0,,	        %Disable%
HKR, NDI\params\htAdhocEnable\enum,1,,	        %Enable%

[htWepTkipOpt.reg]
HKR, Ndi\params\htEnableWepTkip,ParamDesc,  0,  %WepTkip11n%
HKR, NDI\params\htEnableWepTkip,type,,	        "enum"
HKR, NDI\params\htEnableWepTkip,Default,,	"1"
HKR, NDI\params\htEnableWepTkip\enum,0,,	%Disable%
HKR, NDI\params\htEnableWepTkip\enum,1,,	%Enable%

[htEnableWepTkip.reg]
HKR, ,                                  htEnableWepTkip,                  0x00002,  "1"

[cemspecled_func1_1.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[cemspecled_func1_3.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[cemspecled_func1_4.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "8"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[d3forcel1disable.reg]
HKR, ,                                  halPcieWaen,                    0x00002,  "4212539"

[d3forcel1disable1.reg]
HKR, ,                                  halPcieWaen,                         0x00002,  "4212539"
HKR, ,                                  halPcieDetach,                    0x00002,  "1"

[d3forcel1disablekite.reg]
HKR, ,                                  halPcieWaen,                    0x00002,  "4867531"

[d3forcel1disablekite1.reg]
HKR, ,                                  halPcieWaen,                         0x00002,  "4867531"
HKR, ,                                  halPcieDetach,                    0x00002,  "1"

[maxpowersave.reg]
HKR, ,                                  sleepTimePwrSave,               0x00002,  "1000"
HKR, ,                                  SleepTimePerf,                  0x00002,  "1000"

[customer_IODATA.reg]
HKR, ,                  		LinkLedFunc,       		0, "49"
HKR, ,                  		ActivityLedFunc,       		0, "51"

[janusda.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"

[merlinshiftdelay.reg]
HKR, ,                                  analogShiftRegDelay,            0x00002,  "10"

[minpower.reg]
HKR, ,                                  legacyMinTxPowerLimit,            0x00002,  "10"

[wowenable.reg]
HKR, ,                                  wowEnable,                      0x00002,  "1"

[triggerlevelkiteonly.reg]
HKR, ,                                  txTrigLevelMax ,                0x00002,  "32"

[indicaterxlinkspeed.reg]
HKR, ,                                  indicateRxLinkSpeed ,           0x00002,  "1"

;;End of Customized Section

[atheros.Service]
DisplayName     = %ATHR.Service.DispName%
ServiceType     = 1         ;SERVICE_KERNEL_DRIVER
StartType       = 3         ;SERVICE_DEMAND_START
ErrorControl    = 1         ;SERVICE_ERROR_NORMAL
ServiceBinary   = %12%\athr.sys
LoadOrderGroup  = NDIS

[atheros.EventLog]
AddReg = atheros.AddEventLog.reg

[atheros.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


[atheros.CopyFiles]
athr.sys,,,2

[SourceDisksNames]
1 = %DiskDescription%,athr.sys,,

[SourceDisksFiles]
athr.sys = 1,,

[DestinationDirs]
atheros.CopyFiles            = 12
DefaultDestDir               = 11

[Strings]
Msft                         = "Microsoft"
Atheros                      = "Atheros Communications Inc."
Gigabyte                     = "Gigabyte Technology Corp."
ATHR.Service.DispName        = "Atheros Extensible Wireless LAN device driver"
DiskDescription              = "Atheros Sample Driver Disk 1"
TransmitBuffers              = "Transmit Buffers"
ReceiveBuffers               = "Receive Buffers"
NetworkAddress               = "Network Address"
scanTimeValid                = "Scan Valid Interval"
shortPreamble                = "802.11b Preamble"
shortPreambleEnable          = "Long and Short"
shortPreambleDisable         = "Long only"
rssiThrHigh                  = "RSSI Threshold"
rssiThrHighNormal            = "Normal"
rssiThrHighMin               = "Min"
;radioEnable                 = "Radio On/Off"
;radioEnableOn               = "On"
;radioEnableOff              = "Off"
scanTime                     = "Roam Time (sec)"
roamRssiA                    = "Roam Time Threshold (db)"
WirelessMode                 = "Wireless Mode Selection"
WirelessMode11bgOnly         = "802.11b/g"
WirelessModeAuto             = "Auto"
adhocchannel                 = "Adhoc channel Selection"
bkScanEnable                 = "BackgroundScan On/Off"
bkScanEnableOn               = "On"
bkScanEnableOff              = "Off"
radioEnable                  = "Radio On/Off"
radioEnableOn                = "On"
radioEnableOff               = "Off"
roamRssi11A                  = "roamRssiA"
roamRssi11B                  = "roamRssiB"
roamRssi11BOnly              = "roamRssiBOnly"
roamRateA                    = "roamRateA"
roamRateA6M                  = " 6Mbps"
roamRateA9M                  = " 9Mbps"
roamRateA12M                 = "12Mbps"
roamRateA18M                 = "18Mbps"
roamRateA24M                 = "24Mbps"
roamRateA36M                 = "36Mbps"
roamRateA48M                 = "48Mbps"
roamRateA54M                 = "54Mbps"
roamRateBOnly                = "roamRateBOnly"
roamRateBOnly1M              = " 1Mbps"
roamRateBOnly2M              = " 2Mbps"
roamRateBOnly5M              = " 5Mbps"
roamRateBOnly11M             = "11Mbps"
roamRateB                    = "roamRateB"
roamRateB1M                  = " 1Mbps"
roamRateB2M                  = " 2Mbps"
roamRateB5M                  = " 5Mbps"
roamRateB6M                  = " 6Mbps"
roamRateB9M                  = " 9Mbps"
roamRateB11M                 = "11Mbps"
pcieAspm                     = "pcieAspm"
pcieAspmOff                  = "L0s Off, L1 Off"
pcieAspmL0sOn                = "L0s On,  L1 Off"
pcieAspmL1On                 = "L0s Off, L1 On"
pcieAspmL0sandL1On           = "L0s On,  L1 On"
wModeSelect                  = "Wireless Mode"
wModeSelect11bonly           = "11b only"
wModeSelect11nbg             = "11n(2.4GHz) and g and b"
wModeSelect11na              = "11n(5GHz) and a"
wModeSelect11abgn            = "11abgn"
wModeLegacy11a               = "11a only"
wModeLegacy11bonly           = "11b only"
wModeLegacy11bg              = "11g and 11b"
wModeLegacy11abg             = "11abg"
antennaSwitch                = "AntennaSwitch"
antennaSwitchAuto            = "Auto"
antennaSwitchA               = "Antenna A"
antennaSwitchB               = "Antenna B"
Auto			     = "Auto"
5GOnly	                     = "5Ghz Only"
2GOnly	                     = "2Ghz Only"
11DModeSwitch		     = "11d Mode Switch"
Enable			     = "Enable"
Disable                      = "Disable"
WepTkip11n                   = "WepTKIP 11n"
PowerSaveMode		     = "Power Save Mode"
Off			     = "Off"
Maximum                      = "Maximum"
Normal                       = "Normal"
802_11d                      = "802.11d"
smpsDynamic                  = "Dynamic MIMO Power Save"
AdHoc11n                     = "AdHoc 11n"
roamPolicy                   = "Roaming Policy"
roamPolicyVeryHigh           = "Very High"
roamPolicyHigh               = "High"
roamPolicyNormal             = "Normal"
roamPolicyLow                = "Low"
roamPolicyVeryLow            = "Very Low"
ATHR.DeviceDesc.0013         = "Atheros Wireless Network Adapter"
ATHR.DeviceDesc.001A         = "Atheros AR5005G Wireless Network Adapter"
ATHR.DeviceDesc.001B         = "Atheros AR5006X Wireless Network Adapter"
ATHR.DeviceDesc.1030         = "Atheros AR5002G Wireless Network Adapter"
ATHR.DeviceDesc.2030         = "Atheros AR5002G Wireless Network Adapter"
ATHR.DeviceDesc.1031         = "Atheros AR5002X Wireless Network Adapter"
ATHR.DeviceDesc.2031         = "Atheros AR5002X Wireless Network Adapter"
ATHR.DeviceDesc.1041         = "Atheros AR5004G Wireless Network Adapter"
ATHR.DeviceDesc.2041         = "Atheros AR5004G Wireless Network Adapter"
ATHR.DeviceDesc.1042         = "Atheros AR5004X Wireless Network Adapter"
ATHR.DeviceDesc.2042         = "Atheros AR5004X Wireless Network Adapter"
ATHR.DeviceDesc.1051         = "Atheros AR5005GS Wireless Network Adapter"
ATHR.DeviceDesc.2051         = "Atheros AR5005GS Wireless Network Adapter"
ATHR.DeviceDesc.1053         = "Atheros AR5005GS Wireless Network Adapter"
ATHR.DeviceDesc.2053         = "Atheros AR5005GS Wireless Network Adapter"
ATHR.DeviceDesc.1061         = "Atheros AR5006GS Wireless Network Adapter"
ATHR.DeviceDesc.2061         = "Atheros AR5006GS Wireless Network Adapter"
ATHR.DeviceDesc.1062         = "Atheros AR5006XS Wireless Network Adapter"
ATHR.DeviceDesc.2062         = "Atheros AR5006XS Wireless Network Adapter"
ATHR.DeviceDesc.1065         = "Atheros AR5006G Wireless Network Adapter"
ATHR.DeviceDesc.2065         = "Atheros AR5006G Wireless Network Adapter"
ATHR.DeviceDesc.3061         = "Atheros AR5006EGS Wireless Network Adapter"
ATHR.DeviceDesc.3062         = "Atheros AR5006EXS Wireless Network Adapter"
ATHR.DeviceDesc.3063         = "Atheros AR5006EX Wireless Network Adapter"
ATHR.DeviceDesc.3065         = "Atheros AR5006EG Wireless Network Adapter"
ATHR.DeviceDesc.2055         = "Atheros AR5007G Wireless Network Adapter"
ATHR.DeviceDesc.3067         = "Atheros AR5007EG Wireless Network Adapter"
ATHR.DeviceDesc.1071         = "Atheros AR5008 Wireless Network Adapter"
ATHR.DeviceDesc.3072         = "Atheros AR5008X Wireless Network Adapter"
ATHR.DeviceDesc.3091         = "Atheros AR928X Wireless Network Adapter"
ATHR.DeviceDesc.2091         = "Atheros AR922X Wireless Network Adapter"
ATHR.DeviceDesc.30A1         = "Atheros AR9285 Wireless Network Adapter"
ATHR.DeviceDesc.30AA         = "Atheros AR9002WB-1NG Wireless Network Adapter #1"
ATHR.DeviceDesc.30AB         = "Atheros AR9002WB-1NG Wireless Network Adapter #2"
ATHR.DeviceDesc.30A7         = "Atheros AR2427 Wireless Network Adapter"
ATHR.DeviceDesc.10CF         = "IEEE 802.11a/g Wireless LAN Adapter (A)"
ATHR.DeviceDesc.1737_g       = "Linksys Wireless-G Notebook Adapter"
ATHR.DeviceDesc.1737_bg      = "Linksys Wireless A+G Notebook Adapter"
ATHR.DeviceDesc.1737_abg     = "Linksys Wireless A+G PCI Adapter"
ATHR.DeviceDesc.1013         = "11b/g Wireless LAN Mini PCI Adapter"
ATHR.DeviceDesc.2013         = "11a/b/g Wireless LAN Mini PCI Adapter II" 
ATHR.DeviceDesc.3013         = "11b/g Wireless LAN Mini PCI Express Adapter"
ATHR.DeviceDesc.4013         = "11a/b/g Wireless LAN Mini PCI Express Adapter"
ATHR.DeviceDesc.5013         = "11b/g Wireless LAN Mini PCI Express Adapter II"
ATHR.DeviceDesc.6013         = "11b/g Wireless LAN Mini PCI Express Adapter III"
ATHR.DeviceDesc.0032168c     = "11b/g/n Wireless LAN Mini-PCI Express Adapter"
ATHR.DeviceDesc.0033168c     = "11a/b/g/n Wireless LAN Mini-PCI Express Adapter"
ATHR.DeviceDesc.90001385     = "NETGEAR WN711 RangeMax Wireless-N Expresscard Adapter"
ATHR.DeviceDesc.4B001385     = "NETGEAR 108 Mbps Wireless PC Card WG511T"
ATHR.DeviceDesc.5D001385     = "NETGEAR RangeMax(TM) Wireless PC Card WPN511"
ATHR.DeviceDesc.4D001385     = "NETGEAR 108 Mbps Wireless PCI Adapter WG311T"
ATHR.DeviceDesc.4F001385     = "NETGEAR Double 108 Mbps Wireless PC Card WG511U"
ATHR.DeviceDesc.04061468     = "LAN-Express AS IEEE 802.11g miniPCI Adapter"
ATHR.DeviceDesc.04071468     = "LAN-Express AS IEEE 802.11a/g miniPCI Adapter"
ATHR.DeviceDesc.04231468     = "LAN-Express AS IEEE 802.11g PCI-E Adapter"
ATHR.DeviceDesc.F6D3000      = "Belkin Wireless A/G Desktop Network Card"
ATHR.DeviceDesc.80111799     = "Belkin N1 Wireless Notebook Card"
ATHR.DeviceDesc.G650	     = "D-Link AirPlus DWL-G650 Wireless Cardbus Adapter(rev.C)"
ATHR.DeviceDesc.G520X	     = "D-Link AirPlus Xtreme G DWL-G520 Adapter"
ATHR.DeviceDesc.G520	     = "D-Link AirPlus DWL-G520 Wireless PCI Adapter(rev.B)"
ATHR.DeviceDesc.AG520	     = "D-Link AirXpert DWL-AG520 Wireless PCI Adapter"
ATHR.DeviceDesc.AG530	     = "D-Link AirPremier DWL-AG530 Wireless PCI Adapter"
ATHR.DeviceDesc.G630         = "D-Link AirPlus G DWL-G630 Wireless Cardbus Adapter(rev.D)"
ATHR.DeviceDesc.G510	     = "D-Link AirPlus G DWL-G510 Wireless PCI Adapter(rev.B)"
ATHR.DeviceDesc.AG650	     = "D-Link AirXpert DWL-AG650 Wireless Cardbus Adapter"
ATHR.DeviceDesc.AG660	     = "D-Link AirPremier DWL-AG660 Wireless Cardbus Adapter"
ATHR.DeviceDesc.G680         = "D-Link AirPremier DWL-G680 Wireless Cardbus Adapter"
ATHR.DeviceDesc.G550	     = "D-Link AirPremier DWL-G550 Wireless PCI Adapter"
ATHR.DeviceDesc.AG660B	     = "D-Link AirPremier AG DWL-AG660 Wireless Cardbus Adapter"
ATHR.DeviceDesc.AG530B	     = "D-Link AirPremier AG DWL-AG530 Wireless PCI Adapter"
ATHR.DeviceDesc.G650P        = "D-Link AirPlus G DWL-G650+A Wireless Cardbus Adapter"
ATHR.DeviceDesc.G520P	     = "D-Link AirPlus G DWL-G520+A Wireless PCI Adapter"
ATHR.DeviceDesc.WDA1320      = "D-Link WDA-1320 Desktop Adapter"
ATHR.DeviceDesc.WDA2320	     = "D-Link WDA-2320 Desktop Adapter"
ATHR.DeviceDesc.DWA520	     = "D-Link Wireless 108G DWA-520 Desktop Adapter"
ATHR.DeviceDesc.DWA620	     = "D-Link Wireless 108G DWA-620 Notebook Adapter"
ATHR.DeviceDesc.CWNA2330     = "D-Link WNA-2330 Notebook Adapter"
ATHR.DeviceDesc.CWNA1330     = "D-Link WNA-1330 Notebook Adapter"
ATHR.DeviceDesc.CG650        = "D-Link AirPlus Xtreme G DWL-G650 Adapter"
ATHR.DeviceDesc.CG630        = "D-Link AirPlus G DWL-G630 Wireless Cardbus Adapter"
ATHR.DeviceDesc.DWA642       = "D-Link DWA-642 RangeBooster N Notebook Adapter"
ATHR.DeviceDesc.DWA645       = "D-Link DWA-645 RangeBooster N650 Notebook Adapter"
ATHR.DeviceDesc.DWA542       = "D-Link DWA-542 RangeBooster N Desktop Adapter"
ATHR.DeviceDesc.DWA547       = "D-Link DWA-547 RangeBooster N650 Desktop Adapter"
ATHR.DeviceDesc.DWA652       = "D-Link DWA-652 XtremeN Notebook Adapter"
ATHR.DeviceDesc.DWA552       = "D-Link DWA-552 XtremeN Desktop Adapter"
ATHR.DeviceDesc.DWA643       = "D-Link DWA-643 Xtreme N ExpressCard Notebook Adapter"
ATHR.DeviceDesc.DWA556       = "D-Link DWA-556 Xtreme N PCIe Desktop Adapter"
ATHR.DeviceDesc.3070         = "Gigaset PC Card 108"
ATHR.DeviceDesc.3071         = "Speedport Gigaset 54 Mbit"
ATHR.DeviceDesc.800118CB     = "Gigaset PC Card 300"
ATIWC.DeviceDesc.ATICB	     = "Allied Telesyn AT-WCC201g Wireless Card Bus Adapter"
ATIWC.DeviceDesc.ATIPC	     = "Allied Telesyn AT-WCP201g Wireless PCI Adapter"
ATHR.DeviceDesc.2A5F103C     = "Foxconn 802.11 a/b/g/n Wireless System Adaptor"
ATHR.DeviceDesc.500011AD     = "HP 802.11a/b/g Wireless Network Adapter"
ATHR.DeviceDesc.500111AD     = "HP 802.11b/g Wireless Network Adapter"
ATHR.DeviceDesc.1000168c     = "Atheros 802.11 a/b/g/n Dualband Wireless Network Module"
GIGA.DeviceDesc.E914	     = "Gigabyte GN-WI03N (mini) PCI WLAN Card"
GIGA.DeviceDesc.E915	     = "Gigabyte GN-WP02N PCI Express WLAN Card"
GIGA.DeviceDesc.E916	     = "Gigabyte GN-WI06N (mini) PCI Express WLAN Card"
GIGA.DeviceDesc.E815	     = "Gigabyte GN-WM02N Express WLAN Card"
GIGA.DeviceDesc.E801         = "Gigabyte GN-WLMA102 Cardbus WLAN Card"
GIGA.DeviceDesc.E811         = "Gigabyte GN-WMAG Cardbus WLAN Card"
GIGA.DeviceDesc.E814         = "Gigabyte GN-WM01GT Cardbus WLAN Card"
GIGA.DeviceDesc.0013         = "Gigabyte GN-WIAH (mini) PCI WLAN Card"
GIGA.DeviceDesc.E901         = "Gigabyte GN-WI01HT (mini) PCI WLAN Card"
GIGA.DeviceDesc.E911         = "Gigabyte GN-WIAG/GN-WPEAG (mini) PCI WLAN Card"
GIGA.DeviceDesc.E912         = "Gigabyte GN-WP01GT (mini) PCI WLAN Card"
GIGA.DeviceDesc.E913         = "Gigabyte GN-WI01GT (mini) PCI-E WLAN Card"
GIGA.DeviceDesc.E917         = "Gigabyte GN-WI07HT (mini) PCI-E WLAN Card"
GIGA.DeviceDesc.E918         = "Gigabyte GN-WS50G (mini) PCI-E WLAN Card"
GIGA.DeviceDesc.E9191458     = "Gigabyte GN-WS53HN Wireless LAN Mini PCI Express Adapter"
ATHR.DeviceDesc.7141144F     = "Atheros AR9281 Wireless Network Adapter"
ATHR.DeviceDesc.7136144F     = "Atheros AR9280 Wireless Network Adapter"
ATHR.DeviceDesc.E006105B     = "Atheros AR5B91 Wireless Network Adapter"
ATHR.DeviceDesc.CM9          = "WNC CM9 Wireless LAN mini-PCI Network Adapter"
ATHR.DeviceDesc.1ACE         = "TP-LINK Wireless N Adapter"
ATHR.DeviceDesc.00341B0A     = "Atheros AR9281 802.11b/g/n WLAN HMC Network"
ATHR.DeviceDesc.2063         = "Atheros AR5006 802.11a/b/g WiFi Adapter"
ATHR.DeviceDesc.3096         = "Atheros AR5009 802.11a/g/n WiFi Adapter"
ATHR.DeviceDesc.5E001385     = "NETGEAR WPN311 RangeMax(TM) Wireless PCI Adapter"
ATHR.DeviceDesc.0036         = "11b/g/n Wireless LAN Mini-PCI Express Adapter II"
ATHR.DeviceDesc.0037         = "11b/g/n Wireless LAN Mini-PCI Express Adapter III"
ATHR.DeviceDesc.309917AA     = "11a/b/g/n Wireless LAN Adapter"
ATHR.DeviceDesc.7163144F     = "Atheros AR9283 Wireless Network Adapter"
ATHR.DeviceDesc.E01F105B     = "Atheros AR5B93 Wireless Network Adapter"
ATHR.DeviceDesc.663111AD     = "Atheros AR5B95 Wireless Network Adapter"
ATHR.DeviceDesc.30A4         = "Atheros AR9287 Wireless Network Adapter"
ATHR.DeviceDesc.2099         = "Atheros AR9227 Wireless Network Adapter"
ATHR.DeviceDesc.D05B10FC     = "I-O DATA WHG-AGDN/CB Wireless LAN Adapter"

;/* Enable these if VLAN or 802.1p is to be enabled */
;PriorityVLAN                = "Priority & VLAN"
;PriorityVLANDisabled        = "Priority & VLAN Disabled"
;PriorityEnabled             = "Priority Enabled"
;VLANEnabled                 = "VLAN Enabled"
;PriorityVLANEnabled         = "Priority & VLAN Enabled"
